{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":670,"n_cols":9,"rows_kept":670,"merged":[[0,0,0,7],[2,0,32,0],[2,1,32,1],[2,2,32,2],[33,0,39,0],[33,1,39,1],[33,2,39,2],[40,0,72,0],[40,1,72,1],[40,2,72,2],[73,0,88,0],[73,1,88,1],[73,2,88,2],[89,0,90,0],[89,1,90,1],[89,2,90,2],[91,0,93,0],[91,1,93,1],[91,2,93,2],[94,0,96,0],[94,1,96,1],[94,2,96,2],[97,0,104,0],[97,1,104,1],[97,2,104,2],[97,3,104,3],[97,4,104,4],[100,8,103,8],[105,0,125,0],[105,1,125,1],[105,2,125,2],[126,0,147,0],[126,1,147,1],[126,2,147,2],[126,8,128,8],[148,0,149,0],[148,1,149,1],[148,2,149,2],[150,0,156,0],[150,1,156,1],[150,2,156,2],[157,0,174,0],[157,1,174,1],[157,2,174,2],[175,0,177,0],[175,1,177,1],[175,2,177,2],[178,0,185,0],[178,1,185,1],[178,2,185,2],[186,0,216,0],[186,1,216,1],[186,2,216,2],[217,0,223,0],[217,1,223,1],[217,2,223,2],[224,0,237,0],[224,1,237,1],[224,2,237,2],[238,0,255,0],[238,1,255,1],[238,2,255,2],[256,0,263,0],[256,1,263,1],[256,2,263,2],[264,0,266,0],[264,1,266,1],[264,2,266,2],[267,0,282,0],[267,1,282,1],[267,2,282,2],[283,0,310,0],[283,1,310,1],[283,2,310,2],[311,0,314,0],[311,1,314,1],[311,2,314,2],[315,0,331,0],[315,1,331,1],[315,2,331,2],[332,0,345,0],[332,1,345,1],[332,2,345,2],[346,0,369,0],[346,1,369,1],[346,2,369,2],[370,0,416,0],[370,1,416,1],[370,2,416,2],[417,0,426,0],[417,1,426,1],[417,2,426,2],[427,0,441,0],[427,1,441,1],[427,2,441,2],[442,0,448,0],[442,1,448,1],[442,2,448,2],[449,0,455,0],[449,1,455,1],[449,2,455,2],[452,8,455,8],[456,0,465,0],[456,1,465,1],[456,2,465,2],[466,0,467,0],[466,1,467,1],[466,2,467,2],[468,0,469,0],[468,1,469,1],[468,2,469,2],[470,0,473,0],[470,1,473,1],[470,2,473,2],[474,0,486,0],[474,1,486,1],[474,2,486,2],[487,0,488,0],[487,1,488,1],[487,2,488,2],[489,0,492,0],[489,1,492,1],[489,2,492,2],[493,0,507,0],[493,1,507,1],[493,2,507,2],[508,0,512,0],[508,1,512,1],[508,2,512,2],[513,0,517,0],[513,1,517,1],[513,2,517,2],[518,0,529,0],[518,1,529,1],[518,2,529,2],[518,8,529,8],[530,0,536,0],[530,1,536,1],[530,2,536,2],[530,8,536,8],[537,0,551,0],[537,1,551,1],[537,2,551,2],[537,8,551,8],[552,0,560,0],[552,1,560,1],[552,2,560,2],[561,0,593,0],[561,1,593,1],[561,2,593,2],[594,0,608,0],[594,1,608,1],[594,2,608,2],[609,0,669,0],[609,1,669,1],[609,2,669,2],[609,3,643,3],[609,4,643,4],[644,3,656,3],[644,4,656,4],[657,3,661,3],[657,4,661,4],[662,3,669,3],[662,4,669,4]]}
["2024年常用元器件招标标段"]
["序号","标段号","标段内容",null,null,"元器件名称","元器件参数","单位","备注"]
[1,"标段一","电缆头及附件类",null,null,"20kv冷缩电缆准备件","24kV-18/20-3*70","组"]
[{"$nulls":5},"20kV冷缩电缆准备件","24kV-18/20-3*400","组"]
[{"$nulls":5},"10kV冷缩电缆准备件","10kV-3*400","组"]
[{"$nulls":5},"10kV冷缩电缆准备件","10kV-3*70","组"]
[{"$nulls":5},"顶部跨接母线","20kV顶部跨接母线 间距492 (1套含6只丁字头3根母线组装成套)","组"]
[{"$nulls":5},"顶部跨接母线","20kV顶部跨接母线 间距417 (1套含6只丁字头3根母线组装成套)","组"]
[{"$nulls":5},"顶部跨接母线","10kV顶部跨接母线 间距510 (1套含6只丁字头3根母线组装成套)","组"]
[{"$nulls":5},"顶部跨接母线","10kV顶部跨接母线 间距497 (1套含6只丁字头3根母线组装成套)","组"]
[{"$nulls":5},"10kV分段柜连接电缆","12kV（1套含6只前接头,3根单芯300mm2软电缆,连接长度1.5米,组装成套）","套"]
[{"$nulls":5},"10kV分段柜连接电缆","12kV（1套含6只前接头,3根单芯400mm2电缆,连接长度4米,组装成套）","套"]
[{"$nulls":5},"10kV 底部跨接U型母线","15kV/630A 间距375mm  （1套含6只丁字头3根母线组装成套）","套"]
[{"$nulls":5},"10kV 底部跨接U型母线","15kV/630A 间距420mm  （1套含6只丁字头3根母线组装成套）","套"]
[{"$nulls":5},"顶部跨接母线","20kV顶部跨接母线 间距435 (1套含6只丁字头3根母线组装成套)","组"]
[{"$nulls":5},"顶部跨接母线","10kV顶部跨接母线 间距407 (1套含6只丁字头3根母线组装成套)","组"]
[{"$nulls":5},"10kV屏蔽母线(标准化柜用)","15kV/630A  间距700   （1套/3只）","套"]
[{"$nulls":5},"10kV屏蔽母线(标准化柜用)","15kV/630A  间距510  （1套/3只）","套"]
[{"$nulls":5},"10kV屏蔽母线(标准化柜用)","15kV/630A  间距465  （1套/3只）","套"]
[{"$nulls":5},"10kV屏蔽母线(标准化柜用)","15kV/630A  间距420   （1套/3只）","套"]
[{"$nulls":5},"10kV屏蔽母线","15kV/630A  间距375   （1套/3只）","套"]
[{"$nulls":5},"10kV 屏蔽十字接头","15kV/630A  （1套/3只）","套"]
[{"$nulls":5},"10kV 屏蔽型终端接头","15kV/630A  （1套/3只）","套"]
[{"$nulls":5},"PT软连接","（PT连接头及连接线）PT+QJ   中心距900mm（三根）","套"]
[{"$nulls":5},"PT软连接","24kV/630A/中心距900mm（1套含3只前接头3只PT头组装成套）新","套"]
[{"$nulls":5},"电缆附件","电缆前接头24kV/630A,铜芯18/20-3*70mm2（三只/套）新","套"]
[{"$nulls":5},"电缆附件","电缆前接头24kV/630A,铜芯18/20-3*400mm2（三只/套）新","套"]
[{"$nulls":5},"电缆附件","绝缘保护帽630A 24kV/630A（三只/套）新","套"]
[{"$nulls":5},"电缆附件","绝缘保护帽630A 15/630（三只/套）","套"]
[{"$nulls":5},"电缆附件","电缆前接头15kV/630A,铜芯70mm2（三只/套）","套"]
[{"$nulls":5},"电缆附件","电缆前接头15kV/630A,铜芯400mm2（三只/套）","套"]
[{"$nulls":5},"避雷器","24kV屏蔽型后接避雷器 HY5WZ-34/85（1组/3只）新","组"]
[{"$nulls":5},"避雷器","10kV屏蔽型后接避雷器 HY5WZ7-17/45（1组/3只）","组"]
[2,"标段二","隔离、熔断器等手车类",null,null,"隔离手车","10kV 1250A/31.5kA 800mm柜宽 Y0  S8 S9","台"]
[{"$nulls":5},"隔离手车","10kV 1250A/31.5kA 1000mm柜宽 Y0 S8 S9","台"]
[{"$nulls":5},"隔离手车","10kV 4000A/40kA 1000mm柜宽 Y0  S8 S9 带中门闭锁，双侧导轨接地","台"]
[{"$nulls":5},"计量手车","10kV 1250A/25kA 带电度表安装仓 800mm柜宽 Y0  S8 S9，带底盘车闭锁","台"]
[{"$nulls":5},"PT+避雷器手车","安装消谐器、熔断器、避雷器等，800mm宽，10KV 1250A/31.5kA ,S8/S9，带底盘车闭锁","台"]
[{"$nulls":5},"熔断器手车","10kV 1250A/31.5kA 800mm柜宽 Y0 AC/DC220V S8 S9","台"]
[{"$nulls":5},"10kV负荷开关熔断器手车","10kV(带手车闭锁） 1250A   800mm柜宽 Y0  S8 S9","台"]
[3,"标段三","高压互感器类",null,null,"电压互感器PT","20/0.1/0.22 kV，额定容量≥300VA，短时容量≥3000VA/1s，一二次带保护，双熔管,带防雨罩","台","20kV柱上开关ZWBC用"]
[{"$nulls":5},"电流互感器CT","相间距P=380，ABC三相 5P10（0.5），600/5，零序 100/1（工频耐压65/79 kV,雷冲：125/145 kV）（1组A,B,C  3只）","组","20kV柱上开关ZWBC用"]
[{"$nulls":5},"电流互感器CT","电磁式组合传感器:ABC+零三相，600/5A 0.5S（5P10）1VA 100/1A 1S(5P10) 0.5VA 10/√3/6.5/3 3P 2MΩ 1.1Ur ≤20pC，与一体式极柱配合，颜色：国际电工灰 ,每套配12只环氧垫片，3只硅橡胶护套，（每套A,B,C三相）(按照2021版技术新要求）","套","10kV柱上开关ZW32用"]
[{"$nulls":5},"电压互感器PT","JDZW-10R，10/0.1/.0.22kV，10/300VA，0.5/3P级 (按照2021版技术新要求） 配三芯航插，防雨罩。","台"]
[{"$nulls":5},"电流互感器CT","ABC+零一体互感器，5P10（0.5），10VA,零序20/1，3级，0.5VA,200-400-600/5","只","10kV柱上开关ZW20用"]
[{"$nulls":5},"电流互感器","LZZBJ9-12 600/1 0.2S/0.5S/5P20 20/20/30VA","只"]
[{"$nulls":5},"电流互感器","LZZBJ9-10 600/1 0.5/5P20 20/30VA","只"]
[{"$nulls":5},"电流互感器","LZZBJ9-12 600/5A 0.5S 20VA","只"]
[{"$nulls":5},"电流互感器","LZZBJ9-12 500/5 0.2S/0.2S 10/10VA","只"]
[{"$nulls":5},"电流互感器","LZZBJ9-10 400-800/5A 5P30/0.5/0.2S 15/15/15VA 全抽头 国网要求，局放≤5pC，搭接面应镀银，镀银层厚度不小于8um","只"]
[{"$nulls":5},"电流互感器","LZZBJ9-12 100/1 0.5 20VA","只"]
[{"$nulls":5},"电流互感器","LMZB3-10 4000/5A 0.2S/0.5/5P30/5P30/5P30 15/15/15/15/15VA  国网要求，局放≤5pC，搭接面应镀银，镀银层厚度不小于8um","只"]
[{"$nulls":5},"电流互感器","LZZBJ9-10 400/5A 5P30/5P30/0.5/0.2S 20/20/15/15VA","只"]
[{"$nulls":5},"电压互感器","JDZ9-10 10/0.1/0.1 0.2/0.2 30/30VA 全绝缘","只"]
[{"$nulls":5},"电压互感器","JDZXF9-10G2 (10/√3)(0.1/√3)(0.1/√3)(0.1/3) 0.2/0.5/3P 50VA/50VA/100VA 全绝缘","只"]
[{"$nulls":5},"零序互感器","LXK-φ180 100/5 5P10 5VA","只"]
[{"$nulls":5},"电压互感器","三相五柱JSZY18-10FR 10/√3/0.1/√3/0.1/√3/0.1  0.2/0.5/3P 50/50/50VA,配1A熔芯，内置消谐器","只"]
[{"$nulls":5},"电压互感器","JSZV18-20AR  20/0.1/0.22,KX,0.5/3P  50/2*500VA  配1A熔芯","只"]
[{"$nulls":5},"电压互感器","JSZV18-10R  10/0.1/0.1,KX,0.2/0.5  50/50VA  配1A熔芯","只"]
[{"$nulls":5},"电压互感器","JSZW-10NFR  10/√3/0.1/√3/0.22/√3/0.1 ,KX, 0.5/3/3P   30/300/50VA 配1A熔芯（一二次融合用）","只"]
[{"$nulls":5},"电流互感器","LMZK-10 400/5 KX 0.5/10P10(双绕组) 2.5VA/2.5VA","只"]
[{"$nulls":5},"电流互感器","LDZC1365-10 600/5A  0.2S/0.5/5P20(三绕组) 2.5/2.5/2.5VA","只","常州局用"]
[{"$nulls":5},"电流互感器","LDZC1150-10II  100高  100/5A  0.5S  10VA","只"]
[{"$nulls":5},"电流互感器","LDZC1150-10I  55高  600/5A  0.5S  10VA","只"]
[{"$nulls":5},"电流互感器","LMZK1370-20 600/5 KX 0.5/10P10(双绕组) 5VA/5VA","只"]
[{"$nulls":5},"电流互感器","LMZK-10 400/5 KX 0.5/10P10(双绕组) 5VA/5VA","只"]
[{"$nulls":5},"电流互感器","LSZ107-75 600/1,0.5S(5P10) 5VA","只"]
[{"$nulls":5},"电流互感器","LMZK1370-20 600/1 KX 0.5S/5P20(双绕组) 3/3VA  ","只","苏州局配网专用"]
[{"$nulls":5},"零序互感器","LXK-Φ120 100/5,3(10P5), 1VA","只"]
[{"$nulls":5},"零序互感器","LXK-Φ120 20/1,3（10P5), 1VA一二次融合用","只"]
[{"$nulls":5},"零序互感器","LXK-Φ120 100/1,3（10P5),1VA 国网一二次融合用","只"]
[{"$nulls":5},"零序互感器","LXK-Φ120 100/1A，0.5(10P10),容量≥5VA","只","常州地区专用"]
[{"$nulls":5},"零序互感器","LXK-Φ120TH 100/1 KX 5P10 3VA,防水型,线长3m,可固定 ","只","苏州局配网专用"]
[4,"标段四","低压互感器类",null,null,"电流互感器","SDH-0.66-250及以下/5A 0.5","只"]
[{"$nulls":5},"电流互感器","SDH-0.66-400或300/5A 0.5 内孔32*32","只"]
[{"$nulls":5},"电流互感器","SDH-0.66-500~1000/5A 0.5  ","只"]
[{"$nulls":5},"电流互感器","SDH-0.66-2500/5A 0.5 穿100*10双拼铜排 带热缩","只"]
[{"$nulls":5},"电流互感器","SDH-0.66-600/5A 0.5S 穿60X6排，带热缩","只"]
[{"$nulls":5},"电流互感器","SDH-0.66-200~400/5A 0.2S "]
[{"$nulls":5},"电流互感器","SDH-0.66-600/5A 0.2S 穿60*10铜排 带热缩","只"]
[{"$nulls":5},"电流互感器","LMZ1-0.66 2500/5 0.5 穿100*10双拼排 带热缩","只"]
[{"$nulls":5},"电流互感器","LMZ1-0.66 1000~2000/5 0.5  ","只"]
[{"$nulls":5},"电流互感器","LMZ2-0.66 300/5 0.5 穿30*5铜排带热缩","只"]
[{"$nulls":5},"电流互感器","SDH-0.66-400，300，250及以下/5A  内孔32*32 额定冲击耐受电压不小于8kV","只"]
[{"$nulls":5},"电流互感器","ALH-0.66-600/5A  0.5 内孔33*62 额定冲击耐受电压不小于12kV","只"]
[{"$nulls":5},"电流互感器","ALH-0.66-600/5A  内孔62*33 额定冲击耐受电压不小于8kV","只"]
[{"$nulls":5},"电流互感器","LMZ1-0.66 1500/5A 0.2S(5P10) 2.5VA  内孔105*45 额定冲击耐受电压不小于12kV","只"]
[{"$nulls":5},"电流互感器","SDH-0.66-1500~2500/5A 0.5级  内孔102*52 额定冲击耐受电压不小于12kV","只"]
[{"$nulls":5},"电流互感器","SDH-0.66-800/5A 0.5 穿50X10排（矩形，正公差，带热缩）额定冲击耐受电压不小于12kV","只"]
[5,"标段五","接地开关类",null,null,"地刀","JN15-12/31.5KA,含伞齿轮，六角轴，全金属，含传感器，相间距210，≥3000次，铜排搭接面应镀银，镀银层厚度不小于8um","台"]
[{"$nulls":5},"接地开关操作手柄","10KV通用","只"]
[6,"标段六","监测仪、消谐器类",null,null,"监测仪","JCQ5-66","只"]
[{"$nulls":5},"消谐器","LXQIV-10 10KV","只"]
[{"$nulls":5},"消谐器","LXQ-20 10KV","只"]
[7,"标段七","避雷器类",null,null,"避雷器","HY5WZ-17/45","只"]
[{"$nulls":5},"避雷器","HY1.5WS1-0.28/1.3（大电流冲击耐受25kA）","只"]
[{"$nulls":5},"避雷器","HY1.5W-0.28/1.3","只"]
[8,"标段八","浪涌保护器类",null,null,"浪涌保护器","T1试验，标称工作电压（不小于400V），雷电冲击电流（15kA）（10/350µs），带485通讯","只"]
[{"$nulls":5},"浪涌保护器","T1试验，标称工作电压（不小于400V），雷电冲击电流（25kA）（10/350µs），标称放电电流（100kA）（8/20µs），电压保护水平（2.5kV）","只"]
[{"$nulls":5},"浪涌保护器","T2试验，标称工作电压（不小于400V），标称放电电流（不小于40kA）（8/20µs）","只"]
[{"$nulls":5},"浪涌保护器","DC48V 1P直流  15-30KA直流电源防雷器","只","交直流、一体化电源用"]
[{"$nulls":5},"浪涌保护器","20-40KA电涌保护器/SPD浪涌保护器    D级保护  3P+N+PE","只"]
[{"$nulls":5},"浪涌保护器","20-40KA电涌保护器/SPD浪涌保护器    D级保护  1P+N+PE","只"]
[{"$nulls":5},"浪涌保护器","三相电源：C40/3+NPE带故障接点     C级保护","只"]
[{"$nulls":5},"浪涌保护器","放电电流为40KA电涌保护器----单相电源","只"]
[9,"标段九","支架、铁加工件类",null,null,"支架","20KV柱上真空断路器,双PT支架，拼装，具体尺寸详见图纸BCZJ-2402","个"]
[{"$nulls":5},"支架","20KV柱上真空断路器,本体座架,拼装，具体尺寸详见图纸BCZJ-2403","个"]
[{"$nulls":5},"支架","20KV柱上真空断路器,单PT支架,拼装，具体尺寸详见图纸BCZJ-2401","套"]
[{"$nulls":5},"支架","10KV柱上真空断路器，相间距P=340，本体座架,拼装,具体尺寸详见图纸BCZJ-12","套"]
[{"$nulls":5},"支架","10KV柱上真空断路器，PT顶架,热镀锌，喷塑 电气灰RAL 7042，具体尺寸详见图纸BCZJ-02A","套"]
[{"$nulls":5},"支架","单PT支架，拼装，具体尺寸详见图纸BCZJ-14","套"]
[{"$nulls":5},"支架","罩式FTU支架,具体尺寸详见图纸BCZJ-08","套"]
[{"$nulls":5},"支架","双PT支架，拼装具体尺寸详见图纸BCZJ-15","套"]
[{"$nulls":5},"支架","10KV柱上真空断路器，本体座架，拼装,具体尺寸详见图纸BCZJ-13","套"]
[{"$nulls":5},"支架","箱式FTU支架,具体尺寸详见图纸BCZJ-07","套"]
[{"$nulls":5},"外协部分(新JP柜吊装附件)","具体尺寸详见图纸","套"]
[{"$nulls":5},"外协部分(新JP柜圆管焊接附件)--1套1只","具体尺寸详见图纸","套"]
[{"$nulls":5},"外协部分（DP-1-1圆管焊接附件）","具体尺寸详见图纸","套"]
[{"$nulls":5},"外协部分(DP-1-1顶盖)","具体尺寸详见图纸","套"]
[{"$nulls":5},"外协部分(新JP柜底部支架)--1套2根","具体尺寸详见图纸","套"]
[{"$nulls":5},"外协部分(DP-1-1吊装附件)","具体尺寸详见图纸","套"]
[{"$nulls":5},"外协部分(DP-1-1托装支架及附件)","具体尺寸详见图纸","套"]
[{"$nulls":5},"外协部分(出线抱箍及配件)","XLW(出线抱箍及配件)","套"]
[{"$nulls":5},"外协部分(进线抱箍及配件)","XLW(进线抱箍及配件)","套"]
[{"$nulls":5},"外协部分(DP-1-1底部8#槽钢支架)","具体尺寸详见图纸","套"]
[{"$nulls":5},"外协部分(接地装置)",null,"套"]
[10,"标段十","电容器类",null,null,"抽屉式智能电容器","分补，插入式32kvar","只","DP-1标准综合配电箱用"]
[{"$nulls":5},"抽屉式智能电容器","分补，插入式16kvar","只"]
[{"$nulls":5},"抽屉式智能电容器","分补，插入式8+4kvar","只"]
[{"$nulls":5},"控制器","SVG+电容","只"]
[{"$nulls":5},"无功补偿控制器","标准化柜专用","台"]
[{"$nulls":5},"静止无功发生器","30kvar,壁挂式","只"]
[{"$nulls":5},"静止无功发生器模块","30kvar,壁挂式 标准化柜专用","只"]
[{"$nulls":5},"智能电容投切开关","△-30 标准化柜专用","只"]
[{"$nulls":5},"智能电容投切开关","Y-30 标准化柜专用","只"]
[{"$nulls":5},"可控硅晶闸管开关","0.45-30","只"]
[{"$nulls":5},"可控硅晶闸管开关","0.25-30","只"]
[{"$nulls":5},"自愈式电容器","0.45-30-3 标准化柜专用","只"]
[{"$nulls":5},"自愈式电容器","0.25-30-3YN 标准化柜专用","只"]
[{"$nulls":5},"电容器","0.25-20","只"]
[{"$nulls":5},"电容器","0.45-20","只"]
[{"$nulls":5},"智能无功补偿控制器","嵌入式 具数据存储功能，有USB及RS485标准接口,配带电抗电容","台"]
[{"$nulls":5},"智能电力电容器","▲ 450/15~30Kvar带7%电抗，外壳材质不锈钢","只"]
[{"$nulls":5},"智能电力电容器","Y 250/5~20 Kvar带7%电抗，外壳材质不锈钢","只"]
[{"$nulls":5},"智能电力电容器","▲ 450/15~30Kvar 外壳材质不锈钢","只"]
[{"$nulls":5},"智能电力电容器","Y 250/5~20 Kvar 外壳材质不锈钢","只"]
[{"$nulls":5},"智能电力电容器","Y 10 Kvar 内置微断要求分断能力达到15kA","只"]
[{"$nulls":5},"智能电力电容器","Y 20 Kvar   内置微断要求分断能力达到15kA","只"]
[11,"标段十一","变压器类",null,null,"变压器","SCB13-30/10 UK=4.0﹪ 10/0.4kV 30KVA  Dyn11，空载损耗0.15KW 负载损耗0.710KW","台"]
[{"$nulls":5},"变压器","SCB13-30/10 UK=4.0﹪ 10/0.4kV 30KVA  Dyn11  空载损耗0.215KW 负载损耗0.745KW","台"]
[12,"标段十二","温控器类",null,null,"除湿器","15W,AC220V,竖式安装,导轨安装,带RS485接口及故障报警输出接点；满足常州局点表要求,排水管长3米","套"]
[{"$nulls":5},"除湿器","15W,AC220V,竖式安装,导轨安装,排水管长3米.尺寸（宽*高*深）：72*88*50","套"]
[{"$nulls":5},"温湿度控制器","1路温湿度控制,含硅橡胶加热器50W、控制器开孔尺寸45*45、传感器线长4米","套"]
[{"$nulls":5},"温湿度控制器","2路温湿度控制,含铝加热器50W、控制器开孔尺寸45*45、传感器","套"]
[{"$nulls":5},"温控器","拨盘 温度控制器，单路，配传感器，配3米线，AC220V导轨安装，（开孔尺寸45*45mm）","只"]
[{"$nulls":5},"智能除湿装置","AC220V 带报警 排水管长5米 带通讯及报警输出硬接点，带传感器，导轨式安装 15W","台"]
[{"$nulls":5},"温控器","数显，温湿度控制器 双路，配传感器，配3米线，AC220V，（开孔尺寸72*72mm）（带断线报警）面板安装","只"]
[13,"标段十三","熔断器类",null,null,"熔芯","32A（配RT18-32用）","只"]
[{"$nulls":5},"熔芯","4A（配RT18-32用）","只"]
[{"$nulls":5},"熔断器座","RT18-63/3P底座","只"]
[{"$nulls":5},"熔断器座","RT18-63/1P底座","只"]
[{"$nulls":5},"熔断器座","RT18-32/1P底座","只"]
[{"$nulls":5},"熔断器","NT3-300~630A(底座+芯)+RX1-1000（底座+芯）","只"]
[{"$nulls":5},"熔断器","NT1-200A（底座+芯）+RX1-1000（底座+芯）","只"]
[{"$nulls":5},"熔断器","NT00-32A~100A（底座+芯）+RX1-1000（底座+芯）","只"]
[{"$nulls":5},"熔断器","RT18-32/2A~6A","套"]
[{"$nulls":5},"熔断器","RL8B-16/2A","套"]
[{"$nulls":5},"熔断器座","RL8B-16底座","只"]
[{"$nulls":5},"熔断器","NRT16（NT）-00/3P 40A~63三型座","套"]
[{"$nulls":5},"熔断器","NRT16（NT）-00/3P 125A三型座","套"]
[{"$nulls":5},"熔断器","NT00-100/100A","套"]
[{"$nulls":5},"熔断器","NT00-160/125A","套"]
[{"$nulls":5},"高压熔丝","XRNP-12/1A  50KA","只"]
[{"$nulls":5},"高压熔丝","XRNT-10/80A   长292","只"]
[{"$nulls":5},"熔断器夹头","XRNP-12","副"]
[14,"标段十四","静触头类",null,null,"静触头","φ35*84","只"]
[{"$nulls":5},"静触头","φ49*84","只"]
[{"$nulls":5},"静触头","φ49*74","只"]
[15,"标段十五","触头盒、母线套管等绝缘件类",null,null,"套管","202套管","只"]
[{"$nulls":5},"下部套管","环保型下部出线套管","只"]
[{"$nulls":5},"顶部套管","环保型顶部出线套管","只"]
[{"$nulls":5},"绝缘子","φ30*30*M8（环氧）","只"]
[{"$nulls":5},"绝缘子","φ50*50*M8（环氧）","只"]
[{"$nulls":5},"绝缘子","长51mm（孔径Φ6）","只"]
[{"$nulls":5},"母线夹","MD3-80*6/D","只"]
[{"$nulls":5},"母线夹","MD3-60*6/D","只"]
[16,"标段十六","按钮、指示灯、转换开关、行程开关等杂品类",null,null,"LED灯","AC220V,3W,高30mm,宽24mm,长150mm","只"]
[{"$nulls":5},"M16吊耳(配螺栓、平、弹垫)","中置柜","套"]
[{"$nulls":5},"平头带灯按钮","LA38-11D/203 （绿色）一开一闭（自复式）AC220V","只"]
[{"$nulls":5},"按钮","LA38-11/201 绿色,带保护罩","只"]
[{"$nulls":5},"按钮","LA38-11/201（红）","只"]
[{"$nulls":5},"按钮","LA38-22/203 蓝色加防护罩","只"]
[{"$nulls":5},"旋钮","LA38-11X2/201,HS,黑色","只"]
[{"$nulls":5},"按钮附件（透明防护罩带挂锁孔）","AQG7(φ22),HS","只"]
[{"$nulls":5},"按钮附件（透明防护罩）","AQG8(φ22),HS","只"]
[{"$nulls":5},"标字框","孔距40mm,螺丝粗细3mm","只"]
[{"$nulls":5},"指示灯","AD11-22/21-7GZC ","只"]
[{"$nulls":5},"低压电缆抱箍","(55-95)平方毫米","只"]
[{"$nulls":5},"蜂鸣器","AD11-22D/21-CDY, DC110V,HS,红色","只"]
[{"$nulls":5},"行程开关","一开一闭，环网柜用","只"]
[{"$nulls":5},"行程开关","一开一闭，中置柜仪表室用 AC220V","只"]
[{"$nulls":5},"行程开关","YBLX-19/001，中置柜电缆室门用","只"]
[{"$nulls":5},"护角板","2000*400","张"]
[{"$nulls":5},"击穿保险器","JBO 500V","只"]
[{"$nulls":5},"连接片","JL1-2BR2","只"]
[{"$nulls":5},"螺纹卡扣式标字框","孔距35mm,开孔3.5mm","只"]
[{"$nulls":5},"压板","JL1-2BR2","个"]
[{"$nulls":5},"转换开关","LW38D-164D0416/2CY,HS,就地，0°，远方,钥匙通用且仅在远方位时可拔出","只"]
[{"$nulls":5},"转换开关","LW38A-164N5071/1","只"]
[{"$nulls":5},"转换开关","LW38A-164N0393/2","只"]
[{"$nulls":5},"转换开关","LW38DG-164N0393/2","只"]
[{"$nulls":5},"转换开关","LW38E-164N5938/3YS(带不通用鈅匙）","只"]
[{"$nulls":5},"风机+过滤器","TX9805-230（噪音≤55dB）（含TXA50S-172B2H风机）","台","标准化SLVA用"]
[{"$nulls":5},"风机（含底座、金属网）","底座KN-FJ130-X,+风机KN-FJ130","套","标准化DP-1用"]
[{"$nulls":5},"后门电磁锁","DSN-BMY DC/AC110V"]
[{"$nulls":5},"硅胶加热器","JRD-100W  ~220V配6米线","只"]
[{"$nulls":5},"硅胶加热器","JRD-100W  ~220V配3米线","只"]
[17,"标段十七","电流表、电压表类",null,null,"电压表","99T1-V 20/0.1kV,DR,0~24kV","只"]
[{"$nulls":5},"电压表","99T1-V 10/0.1kV,DR","只"]
[{"$nulls":5},"电流表","99T1-A-600/1A,DR","只"]
[{"$nulls":5},"电流表","99T1-A-600/5A,DR","只"]
[{"$nulls":5},"电压表","6L2-V  0~12KV 10/0.1kV","只"]
[{"$nulls":5},"电流表","6L2-A 100/1A","只"]
[{"$nulls":5},"电流表","6L2-A-100/5A","只"]
[18,"标段十八","多功能表、三相表类",null,null,"直流电压表","0~300V AC/DC85V~265V","只"]
[{"$nulls":5},"单相数显电压表","0~300V AC220V","只"]
[{"$nulls":5},"三相数显电压表","AC220（带电压异常告警干接点输出）","只"]
[{"$nulls":5},"直流电流表","直流电流表+/-200~-400A  (带4-20mA) AC/DC85V~265V","只"]
[{"$nulls":5},"直流电流表","直流电流表+/-50~-600A AC/DC85V~265V","只"]
[{"$nulls":5},"三相数显电流表","AC220V（5A）或者(1A)","只"]
[{"$nulls":5},"多功能表","AC/DC220V（信号输入AC380V/5A或者1A,带告警干接点输出，带通讯）","只"]
[{"$nulls":5},"多功能表","带通讯 AC220V 满足国网标准化SLVA相关要求","只"]
[{"$nulls":5},"多功能表","带通讯 AC220V 满足江苏居配501号文","只"]
[{"$nulls":5},"三相电流表","带通讯 AC220V 满足国网标准化SLVA相关要求","只"]
[{"$nulls":5},"三相电流表","带通讯 AC220V 满足江苏居配501号文","只"]
[{"$nulls":5},"电度表","三相四线3*220V/380V，5(60)A 直接表；精度1级","只"]
[{"$nulls":5},"电度表","三相四线3*220V/380V，1.5(6)A 有功0.5S","只"]
[{"$nulls":5},"电压变送器","RTV380/100-T     AC380转100V","只"]
[19,"标段十九","微型断路器类",null,null,"空开","2P,C6A DC","只"]
[{"$nulls":5},"空开","2P,C10A DC","只"]
[{"$nulls":5},"空开","1P,C6A","只"]
[{"$nulls":5},"空开","2P,C6A","只"]
[{"$nulls":5},"空开","3P,C1A","只"]
[{"$nulls":5},"空开","3P,C6A","只"]
[{"$nulls":5},"空开","4P D型 2~125A","只"]
[{"$nulls":5},"空开","4P C型 2~125A","只"]
[{"$nulls":5},"空开","3P D型 10~100A","只"]
[{"$nulls":5},"空开","3P C型 10`100A","只"]
[{"$nulls":5},"空开","2P D型 10~100A","只"]
[{"$nulls":5},"空开","2P C型 2`100A","只"]
[{"$nulls":5},"空开","2P 16~63A DC 三段保护","只"]
[{"$nulls":5},"空开","2P 10~100A DC ","只"]
[{"$nulls":5},"空开","1P 16~100A DC ","只"]
[{"$nulls":5},"辅助触点","OF","只"]
[{"$nulls":5},"报警触点","SD","只"]
[{"$nulls":5},"分励脱扣器","MX","只"]
[20,"标段二十","包装箱类",null,null,"包装箱","柱上真空断路器，相间距P=380，无隔离,填满底板，安装螺栓，尺寸：长1400*宽750*高1000","个"]
[{"$nulls":5},"包装箱","柱上真空断路器，四面围板，盖板，底板另外加长一段","个"]
[{"$nulls":5},"包装箱","柱上真空断路器，相间距P=340，有隔离,填满底板，安装螺栓,尺寸：长1150*宽800*高850","个"]
[{"$nulls":5},"包装箱","柱上真空断路器，相间距P=340，无隔离,填满底板，安装螺栓，长1150*宽630*高850","个"]
[{"$nulls":5},"包装箱","柱上真空断路器，填满底板，安装螺栓，","个"]
[{"$nulls":5},"木底托","分段1分段2柜并柜，详见图纸","个"]
[{"$nulls":5},"木底托","V柜、F柜、C柜、PT柜用，详见图纸","个"]
[{"$nulls":5},"木托盘","型号600X800mm","个"]
[21,"标段二十一","刀熔开关",null,null,"刀熔开关","630/3  630A  SLVA柜专用","只"]
[{"$nulls":5},"刀熔开关","800/3 800A SLVA柜专用","只"]
[{"$nulls":5},"刀熔开关","800/3P,配630A熔芯","只"]
[22,"标段二十二","隔离开关类",null,null,"隔离开关","QAS-160/32,带B型旋转手柄","只"]
[{"$nulls":5},"隔离开关","QP-630A/32带B型旋转手柄(带一开一闭辅助接点)","只"]
[{"$nulls":5},"隔离开关","QP-1000A/32带B型旋转手柄(带一开一闭辅助接点)","只"]
[{"$nulls":5},"隔离开关","QA-630A/22带B型延伸旋转手柄","只"]
[{"$nulls":5},"隔离开关","QA-630A/21带B型延伸旋转手柄","只"]
[{"$nulls":5},"隔离开关","QA-630A/31带H2型旋转手柄","只"]
[{"$nulls":5},"隔离开关","QA-400A/31带B型旋转手柄","只"]
[{"$nulls":5},"隔离开关","QA-400A/22带B型旋转手柄","只"]
[{"$nulls":5},"隔离开关","QA-400A/21带B型旋转手柄","只"]
[{"$nulls":5},"隔离开关","QA-200A/32带B型旋转手柄","只"]
[{"$nulls":5},"隔离开关","QA-200A/21带B型旋转手柄","只"]
[{"$nulls":5},"隔离开关","QA-125A/21带B型旋转手柄","只"]
[{"$nulls":5},"隔离开关","DNH8(HGL)-400/3TM （柜内操作）（配灭弧罩）","只"]
[{"$nulls":5},"隔离开关","DNH8(HGL)-630/3TM （柜内操作）（配灭弧罩）","只"]
[{"$nulls":5},"隔离开关","DNH8(HGL)-400/3JTM （柜外操作）（配灭弧罩）（方杆尺寸定制）","只"]
[{"$nulls":5},"隔离开关","DNH8(HGL)-630/3JTM （柜外操作）（配灭弧罩）（方杆尺寸定制）","只"]
[23,"标段二十三","继电器、交流接触器类",null,null,"SF6气体密度继电器","SF6压力表，SF6带双触点，1付报警、1付低气压闭锁，含自封阀","套"]
[{"$nulls":5},"干燥空气密度继电器","干燥空气压力表,带双触点,1付报警、1付低气压闭锁,含自封阀","套"]
[{"$nulls":5},"继电器","JZX-22FD/2Z插拔式（带底座）","只"]
[{"$nulls":5},"继电器","JTX-2C AC220V（带底座）","只"]
[{"$nulls":5},"继电器","XJ3-G AC380V（带底座）","只"]
[{"$nulls":5},"继电器","JQX-13F/4Z/10A,DC220V(带底座)","只"]
[{"$nulls":5},"继电器","JZ7-44 AC220V","只"]
[{"$nulls":5},"继电器","DY-32/60C 板前接线  整定15～60V","只"]
[{"$nulls":5},"继电器","DY-36/160 板前接线  AC100V,整定40～160V","只"]
[{"$nulls":5},"继电器","JZC1-44Z DC110V","只"]
[{"$nulls":5},"继电器","DZ-31B DC110 板前接线","只"]
[{"$nulls":5},"继电器","JZX54P/L,DC110V,HS,+PYF14A-E","套"]
[{"$nulls":5},"继电器","JZX54P/L,DC48V,HS,+PYF14A-E","套"]
[{"$nulls":5},"信号继电器","DX-31B/DC110 嵌入式","只"]
[{"$nulls":5},"热继电器","25A 与接触器组合  调整范围（17~25A）（AC380V）","只"]
[{"$nulls":5},"交流接触器","63A+线圈电压AC220V(配置两路常开主触头+两路常闭主触头+1常开常闭辅助)","只"]
[{"$nulls":5},"交流接触器","160A可逆型/3P/线圈电压AC220V(含一常开一常闭)","只"]
[{"$nulls":5},"交流接触器","80A可逆型/3P/线圈电压AC220V(含一常开一常闭)+2断电延时","只"]
[{"$nulls":5},"交流接触器","95A可逆型/3P/线圈电压AC220V(含一常开一常闭)","只"]
[{"$nulls":5},"交流接触器","125A可逆型/3P/线圈电压AC220V(含一常开一常闭)","只"]
[{"$nulls":5},"交流接触器","32A可逆型+含一常开一常闭（线圈电压AC220V）","只"]
[{"$nulls":5},"交流接触器","63A可逆型/3P/线圈电压AC220V(含一常开一常闭)+2断电延时","只"]
[{"$nulls":5},"交流接触器","25A+线圈电压AC220V(配置两路常开主触头+两路常闭主触头+1常开常闭辅助)","只"]
[{"$nulls":5},"交流接触器","63A可逆型/3P/线圈电压AC220V(含一常开一常闭)+断电延时","只"]
[{"$nulls":5},"交流接触器附件","断电延时","只"]
[{"$nulls":5},"交流接触器","95A,线圈电源AC220V+2断电延时（AC380V）","套"]
[{"$nulls":5},"交流接触器","63A,线圈电源AC220V+2断电延时（AC380V）","套"]
[{"$nulls":5},"交流接触器","25A+线圈电压AC220V(单相；配置两路常开主触头+两路常闭主触头+1常开常闭辅助)","套"]
[24,"标段二十四","保护装置类",null,null,"保护装置","竖装，10kV线路保护；DC110V/5A，具备CT+合成零序两种保护功能,环网柜用","台"]
[{"$nulls":5},"保护装置","备自投,10KV中置柜用，满足居配要求","台"]
[{"$nulls":5},"保护装置","线路保护,10KV中置柜用，满足居配要求","台"]
[{"$nulls":5},"保护装置","变压器保护,10KV中置柜用，满足居配要求","台"]
[25,"标段二十五","端子类",null,null,"小母线端子","1路（MJ2 ）","只"]
[{"$nulls":5},"电流端子","SKJ-6S","只"]
[{"$nulls":5},"电压端子","UK16N","只"]
[{"$nulls":5},"电压端子","UK10N","只"]
[{"$nulls":5},"电压端子","UK5N","只"]
[{"$nulls":5},"电压端子","UK3N","只"]
[{"$nulls":5},"双层接线端子","SKJ-4/2-2","只"]
[{"$nulls":5},"双层UK5N电压端子","上下层连接片均为顶部连接","只"]
[{"$nulls":5},"电压端子","SKJ-4","只"]
[{"$nulls":5},"电流端子连接件","UFBI 10-RTK/S","条"]
[{"$nulls":5},"插拔式接线端子","4芯，带耳，1套为公母各一只","套"]
[{"$nulls":5},"熔丝端子","ALUK-4RD","只"]
[{"$nulls":5},"普通端子端板","D-UK4/10","袋"]
[{"$nulls":5},"电流端子","URTK-S","只"]
[{"$nulls":5},"普通端子连接件","FBI10-6","条"]
[{"$nulls":5},"端子隔片","TS-K","袋"]
[{"$nulls":5},"胶木端子","TC-1503","只"]
[26,"标段二十六","线鼻、插针类",null,null,"U型线鼻子","1.5-4mm ","袋"]
[{"$nulls":5},"0型线鼻","1.5-4mm","袋"]
[{"$nulls":5},"0型线鼻","2.5-4mm","袋"]
[{"$nulls":5},"插针","1.5 直插式","只"]
[{"$nulls":5},"插针","2.5 直插式","只"]
[{"$nulls":5},"接线鼻","UT1.5-3 直插式","只"]
[{"$nulls":5},"接线鼻","UT2.5-3 直插式","只"]
[{"$nulls":5},"接插件","721-610(公、母)  WAGO","只"]
[{"$nulls":5},"接线鼻","OT10-8","只"]
[{"$nulls":5},"接线鼻","OT2.5-8 直插式","只"]
[{"$nulls":5},"接线鼻","OT2.5-4","只"]
[{"$nulls":5},"接线鼻","OT25-12","只"]
[{"$nulls":5},"接线鼻","OT6-8","只"]
[{"$nulls":5},"接线鼻","OT2.5-8","只"]
[27,"标段二十七","紧固件类",null,null,"M8不锈钢螺柱","304不锈钢，M8*20，尖头。定制","个"]
[{"$nulls":5},"不锈钢弹垫","φ8","只"]
[{"$nulls":5},"不锈钢螺母","M8","只"]
[{"$nulls":5},"不锈钢螺栓","M8*35","只"]
[{"$nulls":5},"不锈钢内六角螺栓","6*40","只"]
[{"$nulls":5},"不锈钢平垫","φ8","只"]
[{"$nulls":5},"抽芯铆钉","6.4*14（带自锁）","只"]
[{"$nulls":5},"点焊螺柱","M6*25","只"]
[{"$nulls":5},"碟形弹簧垫片","φ8","个"]
[{"$nulls":5},"碟形爪垫（白锌）","φ6mm","只"]
[{"$nulls":5},"镀锌弹垫","φ8","只"]
[{"$nulls":5},"镀锌弹垫","φ10","只"]
[{"$nulls":5},"镀锌螺母","M8","只"]
[{"$nulls":5},"镀锌螺母","M10","只"]
[{"$nulls":5},"镀锌螺栓","M8*25","只"]
[{"$nulls":5},"镀锌螺栓","M10*30","只"]
[{"$nulls":5},"镀锌平垫","φ8","只"]
[{"$nulls":5},"镀锌平垫","φ10","只"]
[{"$nulls":5},"镀锌三组合平垫弹垫圆头十一字螺丝","M4*20","只"]
[{"$nulls":5},"镀锌双头螺丝","M6*18","只"]
[{"$nulls":5},"铆螺母","FM8H","只"]
[{"$nulls":5},"内梅花带柱防盗螺栓","304不锈钢M8*40","只"]
[{"$nulls":5},"圆头螺栓","4*25","只"]
[{"$nulls":5},"自攻螺丝","M6*12","只"]
[28,"标段二十八","扎带、线槽、套管等杂品类",null,null,"CT防开路模块","LH-FX-CTB4.1 满足柱上断路器参数要求","个"]
[{"$nulls":5},"PVC防尘罩","气箱202套管用","只"]
[{"$nulls":5},"缠绕管","φ8","卷"]
[{"$nulls":5},"电度表安装支架",null,"只"]
[{"$nulls":5},"电缆夹","小号电缆夹","只"]
[{"$nulls":5},"电缆夹","大号电缆夹","只"]
[{"$nulls":5},"防爆玻璃（加装接地屏蔽层）","长230*宽130*厚13mm","块"]
[{"$nulls":5},"防盗接线盒","DFY-I  三相四线","个"]
[{"$nulls":5},"柜内照明灯(LED)","LL10-W AC220V","只"]
[{"$nulls":5},"环网F柜熔丝筒指示（加厚泡沫胶）","矩形30*25*5（mm)","个"]
[{"$nulls":5},"环网F柜储能指示（加厚泡沫胶）","梯形35*30*5（mm)","个"]
[{"$nulls":5},"环网柜储能指示（加厚泡沫胶）","圆形φ50*5（mm)","个"]
[{"$nulls":5},"环网柜分合闸指示（加厚泡沫胶）","矩形45*45*5（mm)","个"]
[{"$nulls":5},"环氧板","1000*2000*3","张"]
[{"$nulls":5},"环氧板","1000*2000*2","张"]
[{"$nulls":5},"节能灯泡小(含灯座)","3W/220V 白炽灯色","只"]
[{"$nulls":5},"门防火密封条","宽度20mm，厚度8mm","米"]
[{"$nulls":5},"门密封条","宽度15mm，厚度8mm","米"]
[{"$nulls":5},"面板标识框","25*10","套"]
[{"$nulls":5},"尼龙扎带","4*150","只"]
[{"$nulls":5},"尼龙扎带","3*100","只"]
[{"$nulls":5},"平槽","1000mm","根"]
[{"$nulls":5},"绕管","φ12","卷"]
[{"$nulls":5},"塑料袋","透明，密封，A5","只"]
[{"$nulls":5},"塑料护圈","φ30","只"]
[{"$nulls":5},"塑料护圈","φ50","只"]
[{"$nulls":5},"塔型护线套","塔型护线套φ110","只"]
[{"$nulls":5},"线槽","5055","米"]
[{"$nulls":5},"线槽","6030","米"]
[{"$nulls":5},"线槽","8050","米"]
[{"$nulls":5},"相色套管","6mm2","只"]
[{"$nulls":5},"相色套管","10mm2","根"]
[{"$nulls":5},"相色套管","16mm2 ","只"]
[{"$nulls":5},"相色套管","25mm2","米"]
[{"$nulls":5},"相色套管","35mm2","只"]
[{"$nulls":5},"橡皮圈","φ150","只"]
[{"$nulls":5},"橡皮圈","φ120","只"]
[{"$nulls":5},"橡皮圈","φ50","只"]
[{"$nulls":5},"橡皮圈","φ30","只"]
[{"$nulls":5},"中扎带","4*150","袋"]
[{"$nulls":5},"扎带","5*300","袋"]
[{"$nulls":5},"扎带","3*150","袋"]
[{"$nulls":5},"字套管（圆管，内防滑）","50","公斤"]
[{"$nulls":5},"字套管","LP-25.0","米"]
[{"$nulls":5},"字套管","LP-16.0","米"]
[{"$nulls":5},"字套管","LP-10.0","米"]
[{"$nulls":5},"字套管","H0-80","卷"]
[29,"标段二十九","铰链、锁具类",null,null,"铰链","HL035-2","副"]
[{"$nulls":5},"铰链","HL051-3.1","副"]
[{"$nulls":5},"铰链","HL012","副"]
[{"$nulls":5},"计量锁","MS505(左开)","把"]
[{"$nulls":5},"门锁","MS705-1-2（H=22）","把"]
[{"$nulls":5},"防雨锁","MS887-2(单点锁片）","把"]
[{"$nulls":5},"门锁","MS414,锁舌折弯","把"]
[{"$nulls":5},"把手","PL006","只"]
[{"$nulls":5},"把手","PL004-3","只"]
[{"$nulls":5},"三爪不锈钢铰链","20/M8*12","副"]
[30,"标段三十","独股/多股铜芯线类/蔽线类",null,null,"二芯屏蔽线","RVVP 2*0.75","米"]
[{"$nulls":5},"二芯屏蔽线","RVVP2*0.3","米"]
[{"$nulls":5},"二芯屏蔽线","RVVP 2*0.5","米"]
[{"$nulls":5},"三芯屏蔽线","RVVP3*0.75 芯线颜色黄绿红","米"]
[{"$nulls":5},"多股铜芯线","ZR-BVR-1","米"]
[{"$nulls":5},"多股铜芯线","ZR-BVR-1.5 ","米"]
[{"$nulls":5},"多股铜芯线","ZR-BVR-2.5","米"]
[{"$nulls":5},"多股铜芯线","ZR-BVR-4.0 ","米"]
[{"$nulls":5},"多股双色线（黄绿线）","ZR-BVR-6","米"]
[{"$nulls":5},"多股铜芯线","ZR-BVR-10","米"]
[{"$nulls":5},"多股铜芯线","ZR-BVR-16","米"]
[{"$nulls":5},"多股铜芯线","ZR-BVR-25","米"]
[{"$nulls":5},"多股铜芯线","ZR-BVR-35","米"]
[{"$nulls":5},"多股铜芯线","ZR-BVR-50","米"]
[{"$nulls":5},"独股铜芯线","ZR-BV-4","米"]
[31,"标段三十一","标牌类",null,null,"铭牌","125*80*0.5","块"]
[{"$nulls":5},"铭牌","125*80*0.6","块"]
[{"$nulls":5},"铭牌","200*50*2有机玻璃 江苏省居配项目专用 2019新款","块"]
[{"$nulls":5},"铭牌","150*90*0.5","块"]
[{"$nulls":5},"铭牌","160*100*0.5","块"]
[{"$nulls":5},"铭牌和二维码一体式标牌","200*124*0.6 国网标准化低压柜用","块"]
[{"$nulls":5},"铭牌","125*80*0.8","块"]
[32,"标段三十二","控制器/DTU/FTU",null,null,"控制器FTU","罩式控制器能实现三段保护，24V,有后备电源，配三遥，公专一体4G无线通讯模块,硬加密，具有故障查询功能，10M。","台"]
[{"$nulls":5},"控制器FTU(一二次融合）","罩式FTU, 24V,有后备电源，8米线缆,满足一二次融合要求，需全检,(按照2021版技术新要求:标准化）","台"]
[{"$nulls":5},"控制器FTU","箱式控制器能实现三段保护，24V,有后备电源，配三遥，公专一体4G无线通讯模块,硬加密，具有故障查询功能，增加独立的操作电源回路开关；线缆10M。","台"]
[{"$nulls":5},"环网柜智能开关控制器","ISCU-P03(预储能V机构),DC110V,带透明罩","套","技术参数要求不低于厂家-福建国青"]
[{"$nulls":5},"环网柜智能开关控制器","ISCU-P01(C机构/F机构),带透明罩","只"]
[{"$nulls":5},"环网柜智能开关控制器","ISCU-P02/48-S 三挡位转换开关,合闸按钮及指示灯为红色,分闸按钮及指示灯为绿色,带透明罩,苏州局配网专用","只"]
[{"$nulls":5},"环网柜智能开关控制器","ISCU-P03/48-S 三挡位转换开关,合闸按钮及指示灯为红色,分闸按钮及指示灯为绿色,带透明罩,苏州局配网专用","只"]
[33,"标段三十三","航空插头插座类",null,null,"矩形航空插头+电缆(蓝色间隔6)","含1只间隔柜端32芯插头、1只DTU端26芯插头，1根长度7m的电缆，带防呆设计，颜色：蓝色(间隔6)，满足一二次融合新标准规范要求。","套"]
[{"$nulls":5},"矩形航空插头+电缆(黄色间隔5)","含1只间隔柜端32芯插头、1只DTU端26芯插头，1根长度6.5m的电缆，带防呆设计，颜色：黄色(间隔5)，满足一二次融合新标准规范要求。","套"]
[{"$nulls":5},"矩形航空插头+电缆(绿色间隔4)","含1只间隔柜端32芯插头、1只DTU端26芯插头，1根长度6m的电缆，带防呆设计，颜色：绿色(间隔4)，满足一二次融合新标准规范要求。","套"]
[{"$nulls":5},"矩形航空插头+电缆(红色间隔3)","含1只间隔柜端32芯插头、1只DTU端26芯插头，1根长度5.5m的电缆，带防呆设计，颜色：红色(间隔3)，满足一二次融合新标准规范要求。","套"]
[{"$nulls":5},"矩形航空插头+电缆(白色间隔2)","含1只间隔柜端32芯插头、1只DTU端26芯插头，1根长度5m的电缆，带防呆设计，颜色：白色(间隔2)，满足一二次融合新标准规范要求。","套"]
[{"$nulls":5},"矩形航空插头+电缆(黑色间隔1)","含1只间隔柜端32芯插头、1只DTU端26芯插头，1根长度4.5m的电缆，带防呆设计，颜色：黑色(间隔1)，满足一二次融合新标准规范要求。","套"]
[{"$nulls":5},"矩形航空插头+电缆(PT间隔)","含1只PT柜端32芯插头、1只DTU端32芯插头，1根长度4m的电缆，带防呆设计，颜色：黑色(PT柜)，满足一二次融合新标准规范要求。","套"]
[{"$nulls":5},"航空插头插座","航空插头插座，YD41-26ZJ/TK-0.9*，含防尘罩，铝，直，全引脚方案","只"]
[{"$nulls":5},"航空插头插座短路环","6芯短路环","只"]
[{"$nulls":5},"航空插座","航空插座，GM16密封端子板/TK-0.9*，全引脚方案","套"]
[34,"标段三十四","灭弧室类",null,null,"灭弧室","灭弧室，24KV,630A-20kA,  工频耐压65/79 kV,雷冲：125/145 kV","只","20KV柱上断路器ZWBC-24用"]
[{"$nulls":5},"灭弧室","灭弧室，12KV,630A-20kA，与一体化绝缘筒配套,工频耐压42/48 kV,雷冲：75/85 kV","只","10KV柱上断路器ZW32-12用"]
[35,"标段三十五","固封极柱",null,null,"固封极柱","12KV/4000A-40KA，配矮散热架(BV7.128.517) 柜内真空断路器用","只"]
[{"$nulls":5},"固封极柱","12KV/1250A-31.5KA 柜内真空断路器用","只"]
[36,"标段三十六","ZW20/32散件、隔离开关类",null,null,"散件","相间距P=380，散件，电动  进出线桩头镀锡层厚度12μm","台","20KV柱上断路器ZWBC-24用"]
[{"$nulls":5},"隔离开关","相间距P=380,（整个隔离刀导电回路镀锡层厚度12μm）","套","20KV柱上断路器ZWBC-24用"]
[{"$nulls":5},"散件","相间距P=340，一体化极柱散件，电动, IP65,  进出线桩头镀锡层厚度12μm，（弹簧座Φ38），铜棒长度245mm.配铝垫块(厚度10mm), (按照2021版技术新要求）.","套"]
[{"$nulls":5},"隔离开关","相间距P=340,一体化极柱隔离刀，配垫块9cm（整个隔离刀导电回路镀锡层厚度12μm），隔离刀侧需安装零序电压传感器，需留安装孔,热镀锌","套"]
[37,"标段三十七","操作机构类",null,null,"操作机构","操作机构，电动， 24V（大行程）","个","20KV柱上断路器ZWBC-24用"]
[{"$nulls":5},"操作机构","操作机构，电动，24V(按照2021版技术新要求）","个","10KV柱上断路器ZW32-12用"]
[{"$nulls":5},"20kV负荷开关-熔断器组合操作机构","20KV,电动DC48V，硬联锁，含动密封、螺柱安装包，配熔丝筒脱扣硬联锁组件,下门挂销长度25mm,配二次线，接点灌胶","套"]
[{"$nulls":5},"环保型断路器+上隔离开关操作机构","环保型,断路器电动DC48V,隔离手动,硬联锁，含动密封,含面板操作按钮，配二次线且桩头灌胶","套"]
[{"$nulls":5},"断路器隔离开关操作机构","手动，硬联锁，含动密封、螺柱安装包,配二次线且桩头灌胶出厂，下门挂销长度33mm（程序锁,交叉互锁；配2把锁）","套"]
[{"$nulls":5},"断路器隔离开关操作机构","手动，硬联锁，含动密封、螺柱安装包，配二次线且桩头灌胶，下门挂销长度33mm;（程序锁,配1把锁）","套"]
[{"$nulls":5},"20kV断路器隔离开关操作机构","20kV,手动，硬联锁，含动密封、螺柱安装包，配二次线，接点灌胶，下门挂销长度33mm","套"]
[{"$nulls":5},"20kV断路器操作机构","20kV,电动DC48V,含动密封,配二次线，接点灌胶","套"]
[{"$nulls":5},"20kV负荷开关操作机构","20kV,电动DC48V，硬联锁，含动密封、螺柱安装包,配二次线且桩头灌胶，下门挂销长度33mm","套"]
[{"$nulls":5},"负荷开关操作机构","电动DC110V，硬联锁，含动密封、螺柱安装包,配二次线且桩头灌胶出厂，下门挂销长度33mm（程序锁,交叉互锁；配3把锁）","套"]
[{"$nulls":5},"断路器操作机构","电动DC48V,含动密封,配二次线且桩头灌胶","套"]
[{"$nulls":5},"负荷开关-熔断器组合操作机构","电动DC110V，硬联锁，含动密封、螺柱安装包，配熔丝筒脱扣硬联锁组件,下门挂销长度25mm,配二次线且桩头灌胶","套"]
[{"$nulls":5},"环保型断路器+上隔离开关","环保型,630A-20kA，三工位,上隔离,极柱式断路器","套"]
[38,"标段三十八","ZW20/32壳体类",null,null,"壳体","相间距P=380，壳体304不锈钢(实测厚度≥3mm)，喷塑(含接线盒)，PT螺柱，防开路模块安装板，电子标签安装板。（6个面含封板采用304不锈钢实测厚度≥3mm，正公差板材）","台","20KV柱上断路器ZWBC-24用"]
[{"$nulls":5},"壳体","相间距P=340，壳体304不锈钢(实测厚度≥3.0mm),一体化极柱，IP65,喷塑颜色:RAL7042，PT螺柱，CT支架螺柱，接线盒,防开路模块安装板，配三相电流互感器,CT支撑支架.（6个面含封板采用304不锈钢实测厚度≥3mm，正公差板材）","套"]
[39,"标段三十九","机构组件",null,null,"机构组件(储能（AC/DC220V）分合闸线圈（AC/DC220V）；合闸闭锁（AC/DC220V）；防跳；手车闭锁（AC/DC220V）","10KV柜内真空断路器 630A/25KA，封板、推板、触臂、梅花触头30片（镀银层8um）不配底盘车","套"]
[{"$nulls":5},"机构组件(储能（AC/DC220V）分合闸线圈（AC/DC220V）；合闸闭锁（AC/DC220V）；防跳；手车闭锁（AC/DC220V）","10KV柜内真空断路器 1250A/25KA~31.5kA，封板、推板、触臂、梅花触头30片（镀银层8um）不配底盘车","套"]
[{"$nulls":5},"机构组件(储能（AC/DC 220V）分合闸线圈（AC/DC 220V）；合闸闭锁（AC/DC 220V）；防跳；手车闭锁（AC/DC 220V）","10KV柜内真空断路器  4000A/40kA，封板、推板、触臂、梅花触头84片（镀银层8um）,不配底盘车","套"]
[{"$nulls":5},"机构组件(储能电机AC/DC220V;分合闸线圈（AC/DC220V）；合闸闭锁（AC/DC220V）；手车闭锁（AC/DC220V），带防跳)","20KV柜内真空断路器  630~1250A/25kA，封板、推板、触臂、梅花触头24片（镀银层8um）,无需配底盘车","套"]
[40,"标段四十","带电显示器/故障指示器类/综合状态指示仪",null,null,"带电显示器","DXN-12/Q,DC48V,15pF, 92*44","套"]
[{"$nulls":5},"带电显示器","DXN-12/Q,DC110V,15pF, 92*44,带核相功能","套"]
[{"$nulls":5},"带电显示器","DXN-12/Q,DC110V,15pF, 92*44 带自检","套"]
[{"$nulls":5},"带电显示器","DXN-12/T,15pF, 92*44","套"]
[{"$nulls":5},"带电显示器","DXN-24/T,15pF, 92*44","套"]
[{"$nulls":5},"带电显示器","DXN-24/Q,DC48V,15pF, 92*44","套"]
[{"$nulls":5},"带电显示器","DXN8D-12/T4S  (高分用）","只"]
[{"$nulls":5},"带电显示器","DXN-12kV/Q14， AC/DC110V,2个闭锁，带自检,带验电,带核相功能,开孔尺寸92X44 (核相插孔口径统一为4mm)","只"]
[{"$nulls":5},"综合状态指示仪","10kV(不带带电显示功能，不带除湿加热功能，仅带开关状态指示功能）带报警接点","只"]
[{"$nulls":5},"核相器","10kV核相器","套"]
[{"$nulls":5},"核相器","20kV核相器","套"]
[{"$nulls":5},"故障指示器（面板型）","EKL4   配3米电缆光纤（高分用）","套"]
[{"$nulls":5},"故障指示器","TSEC-I带测温和故障报警，配光纤6米（KYN28A-12用），接地和短路故障分项显示","套"]
[{"$nulls":5},"故障指示器","EKL-4,3米光纤,24kV用","套"]
[{"$nulls":5},"故障指示器","EKL-4,3米光纤,12kV用","套"]
[41,"标段四十一","ZW20/32/BC绝缘件",null,null,"绝缘件","20KV柱上真空断路器，相间距P=380，含A,B,C三相，配黄绿红护套","台"]
[{"$nulls":5},"绝缘件","相间距P=340，一体化极柱（颜色：RAL7042）及绝缘附件, (按照2021版技术新要求）.含黄绿红护套,隔离护套。","套"]
[{"$nulls":5},"ZW20绝缘盒密封圈","10KV柱上真空断路器，绝缘盒密封圈（软质硅橡胶）","个"]
[{"$nulls":5},"绝缘件","10KV柱上真空断路器0，含黄绿红护套,进出线端子镀锡层厚度 12μm,进出线带伞裙，大罩需开孔","套"]
[{"$nulls":5},"20KV柱开绝缘护套","20KV柱开绝缘护套（隔离护套，桩头护套，黄绿红）","套"]
[42,"标段四十二","10KV断路器类",null,null,"断路器","10KV柜内真空断路器  1250A/31.5kA 储能电机DC110，手车闭锁DC110，分合闸线圈DC110，合闸闭锁DC110，带防跳，手车式，固封极柱，带底盘车闭锁","台"]
[{"$nulls":5},"三锁二钥匙","三锁二钥匙 配套10KV柜内真空断路器","套"]
[{"$nulls":5},"三锁三钥匙","三锁三钥匙 配套10KV柜内真空断路器","套"]
[{"$nulls":5},"分闸线圈","与10KV柜内真空断路器配套,DC110V","个"]
[{"$nulls":5},"合闸线圈","与10KV柜内真空断路器配套,DC110V","个"]
[43,"标段四十三","剩余电流断路器，塑壳断路器（低分和JP专用)",null,null,"剩余电流动作断路器","额定运行短路分断能力≥35KA,3P+N 160A 含相间隔板 带重合闸功能","台","详见技术规范要求"]
[{"$nulls":5},"塑壳断路器","额定极限分断能力50KA,3P 400A 含相间隔板","台"]
[{"$nulls":5},"相间隔板","配250","片"]
[{"$nulls":5},"塑壳断路器","额定极限分断能力50KA,400A/3P 带通讯新规约，含相间隔板","台"]
[{"$nulls":5},"塑壳断路器","额定极限分断能力50KA,630A/3P 带通讯新规约，含相间隔板","台"]
[{"$nulls":5},"塑壳断路器","额定极限分断能力50KA,250A/3P 带通讯新规约，含相间隔板和过渡铜排","台"]
[{"$nulls":5},"塑壳断路器","额定极限分断能力50KA,250A/3P","台"]
[{"$nulls":5},"剩余电流动作断路器","额定运行短路分断能力≥35KA,400A,3P+N带通讯接口(新规约）含相间隔板 具备突变剩余动作电流30～75mA可调功能","台"]
[{"$nulls":5},"剩余电流动作断路器","额定运行短路分断能力≥35KA,630A,3P+N带通讯接口(新规约）含相间隔板 具备突变剩余动作电流30～75mA可调功能","台"]
[{"$nulls":5},"剩余电流动作断路器","额定运行短路分断能力≥35KA,400A,3P+N带通讯接口(新规约）含相间隔板 具备突变剩余动作电流30～75mA可调功能 标准化DP-1用","台"]
[{"$nulls":5},"剩余电流动作断路器","额定运行短路分断能力≥50KA,630A,3P+N带通讯接口(新规约）含相间隔板 具备突变剩余动作电流30～75mA可调功能 标准化DP-1用","台"]
[{"$nulls":5},"塑壳断路器","额定极限分断能力50KA,250A/3P 带通讯新规约，含相间隔板","台"]
[44,"标段四十四","框架塑壳断路器 符合SLVA标准化低压柜中断路器部分的要求",null,null,"塑壳断路器","GM8-800H/3E  630A  2AX  插入式板后接线  带通讯新规约  标准化柜专用","台","技术参数要求不低于北京人民"]
[{"$nulls":5},"框架断路器","GW6-32N25 3D2 GER3 5.0A+SDE 485通讯(DL/T 645江苏新规约) AC220V,6NO+6NC,电源模块,三位置指示器,垂直母线,含相间隔板和门框  标准化柜专用","台"]
[{"$nulls":5},"框架断路器","GW6-20H06 3D2 GER3 5.0A+SDE 485通讯 AC220V,4NO+4NC,电源模块,三位置指示器,垂直母线,含相间隔板和门框  标准化柜专用","台"]
[{"$nulls":5},"塑壳断路器","GM8-125H/3E 63A","台"]
[{"$nulls":5},"塑壳断路器","GM8-400H/3E  250A~400A 2AX  带通讯新规约  标准化柜专用","台"]
[{"$nulls":5},"塑壳断路器","GM8-800H/3E  630A  2AX  带通讯新规约  标准化柜专用","台"]
[{"$nulls":5},"三锁二钥匙","配GW6断路器用","套"]
[45,"标段四十五","框架塑壳断路器（居配低压柜）  ",null,null,"框架断路器","额定工作电压400V,额定极限分断能力和额定运行分断能力65KA,机械寿命（免维护）≥10000次,额定冲击耐受电压12kV,2000/4P 1000A 抽屉式 液晶四遥，AC220V 无欠压，六开六闭","台","技术参数满足501文件要求"]
[{"$nulls":5},"框架断路器","额定工作电压660V,额定极限分断能力和额定运行分断能力65KA,机械寿命（免维护）≥10000次,额定冲击耐受电压12kV,3P 2500A 抽屉式 液晶四遥 无欠压220V 六开六闭","台"]
[{"$nulls":5},"框架断路器","额定工作电压660V,额定极限分断能力和额定运行分断能力65KA,机械寿命（免维护）≥10000次,额定冲击耐受电压12kV,3P 2500A 抽屉式 液晶四遥，AC220V 无欠压，四常开四常闭","台"]
[{"$nulls":5},"三锁二钥匙","配套框架断路器","套"]
[{"$nulls":5},"七锁四钥匙","配套框架断路器","套"]
[{"$nulls":5},"二锁一钥匙","配套框架断路器","套"]
[{"$nulls":5},"相间隔板","配250","片"]
[{"$nulls":5},"塑壳断路器","额定工作电压400V,额定极限分断能力和额定运行分断能力50KA,机械寿命（免维护）≥10000次,电气寿命≥7000次,额定冲击耐受电压8kV,630A/3P,插拔式板前,含相间隔板","台"]
[{"$nulls":5},"塑壳断路器","额定工作电压400V,额定极限分断能力和额定运行分断能力50KA,机械寿命（免维护）≥10000次,电气寿命≥7000次,额定冲击耐受电压8kV,630A/3P,含相间隔板","台"]
[{"$nulls":5},"塑壳断路器","额定工作电压400V,额定极限分断能力和额定运行分断能力50KA,机械寿命（免维护）≥10000次,电气寿命≥7000次,额定冲击耐受电压8kV,400A/3P 插入式板前","台"]
[{"$nulls":5},"塑壳断路器","额定工作电压400V,额定极限分断能力和额定运行分断能力50KA,机械寿命（免维护）≥10000次,电气寿命≥7000次,额定冲击耐受电压8kV,400A/3P 带通讯新规约 AC220V分励辅助配线长1.2m","台"]
[{"$nulls":5},"塑壳断路器","额定工作电压400V,额定极限分断能力和额定运行分断能力50KA,机械寿命（免维护）≥10000次,电气寿命≥7000次,额定冲击耐受电压8kV,400A/3P含辅助接点 含相间隔板","台"]
[{"$nulls":5},"塑壳断路器","额定工作电压400V,额定极限分断能力和额定运行分断能力50KA,机械寿命（免维护）≥10000次,电气寿命≥7000次,额定冲击耐受电压8kV,160A/3P 含辅助接点 含相间隔板","台"]
[{"$nulls":5},"塑壳断路器","额定工作电压400V,额定极限分断能力和额定运行分断能力50KA,机械寿命（免维护）≥10000次,电气寿命≥7000次,额定冲击耐受电压8kV,250A/3P带通讯新规约 AC220V分励辅助配线长1.2m","台"]
[{"$nulls":5},"塑壳断路器","额定工作电压400V,额定极限分断能力和额定运行分断能力50KA,机械寿命（免维护）≥10000次,电气寿命≥7000次,额定冲击耐受电压8kV,125A/3P","台"]
[46,"标段四十六","双电源切换开关",null,null,"ATS","CB级  250A/3P","只"]
[{"$nulls":5},"ATS","CB级  63A/4P","只"]
[{"$nulls":5},"ATS","PC级 630A/3P","只"]
[{"$nulls":5},"ATS","PC级 400A/3P","只"]
[{"$nulls":5},"ATS","PC级 320A/3P","只"]
[{"$nulls":5},"ATS","PC级 250A/3P","只"]
[{"$nulls":5},"ATS","PC级 200A/3P","只"]
[{"$nulls":5},"ATS","PC级 63A/3P","只"]
[{"$nulls":5},"智能控制器","ATS智能控制器","只"]
[47,"标段四十七","交直流电源柜用断路器",null,null,"框架断路器","2000壳架800A/3P/AC400V抽屉式 操作电压DC220V，6常开6常闭，双报警，门框，相间隔板","台"]
[{"$nulls":5},"框架断路器","2000壳架1000A/3P/AC400V 抽屉式 操作电压DC220V，6常开6常闭，双报警，门框，相间隔板","台"]
[{"$nulls":5},"框架断路器","1600壳架/630A抽屉式/3极/操作电压DC220V，6常开6常闭，双报警，门框，相间隔板","台"]
[{"$nulls":5},"框架断路器","1600壳架/800A抽屉式/3极/操作电压DC220V，6常开6常闭，双报警，门框，相间隔板","台"]
[{"$nulls":5},"塑壳断路器","800壳架  800A/3/带辅助报警触头(电子式、50KA)","台"]
[{"$nulls":5},"塑壳断路器","630壳架  630A/3/带辅助报警触头(热磁、分励AC220V、电动机保护)","台"]
[{"$nulls":5},"塑壳断路器","630壳架  630A/3/带辅助报警触头(热磁、电动机保护)","台"]
[{"$nulls":5},"塑壳断路器","630壳架   630A/3/带辅助报警触头(热磁、配电保护)","台"]
[{"$nulls":5},"塑壳断路器","630壳架   630A/3/带辅助报警触头(电子式、50KA)","台"]
[{"$nulls":5},"塑壳断路器","630壳架 400A/2/带报警触头；直流","台"]
[{"$nulls":5},"塑壳断路器","630壳架  315A/2/带辅助报警触头(热磁、配电保护)*2+机械连锁SHS-II","台"]
[{"$nulls":5},"塑壳断路器","400壳架  400A/3/带辅助报警触头(电子式、50KA)","台"]
[{"$nulls":5},"塑壳断路器","400壳架  400A/3/带辅助报警触头(热磁、配电保护)","台"]
[{"$nulls":5},"塑壳断路器","400壳架  400A/3/双辅助触头，报警触头(热磁)","台"]
[{"$nulls":5},"塑壳断路器","250壳架  250A/3/带通讯适配器（报警与辅助）带操作手柄","台"]
[{"$nulls":5},"塑壳断路器","250壳架  250A/3/带通讯适配器（报警与辅助）","台"]
[{"$nulls":5},"塑壳断路器","250壳架 250A/2/带辅助报警触头(直流；三段式保护)","台"]
[{"$nulls":5},"塑壳断路器","250壳架  250A/3/带辅助触头(热磁)","台"]
[{"$nulls":5},"塑壳断路器","250壳架 250A/3/带辅助报警触头(热磁、配电保护)","台"]
[{"$nulls":5},"塑壳断路器","250壳架 200A/2/带辅助报警触头；直流","台"]
[{"$nulls":5},"塑壳断路器","250壳架  200A/3/带辅助报警触头(电子式、50KA)","台"]
[{"$nulls":5},"塑壳断路器","250壳架 200A/2/带辅助报警触头；直流*2+机械联锁","台"]
[{"$nulls":5},"塑壳断路器","250壳架  160A/3/带辅助和报警触头","台"]
[{"$nulls":5},"塑壳断路器","250壳架  160A/3/带辅助报警触头(热磁、分励AC220V、电动机保护)","台"]
[{"$nulls":5},"塑壳断路器","250壳架  160A/3/带辅助报警触头(热磁、电动机保护)","台"]
[{"$nulls":5},"塑壳断路器","250壳架 160A/3(热磁、配电保护)","台"]
[{"$nulls":5},"塑壳断路器","125壳架  125A/3/带通讯适配器（报警与辅助）","台"]
[{"$nulls":5},"塑壳断路器","125壳架  125A/3/带通讯适配器（报警与辅助）带操作手柄","台"]
[{"$nulls":5},"塑壳断路器","125壳架 125A/2/带辅助报警触头(直流；三段式保护)","台"]
[{"$nulls":5},"塑壳断路器","125壳架  125A/3/带辅助报警触头(热磁、分励AC220V、电动机保护)","台"]
[{"$nulls":5},"塑壳断路器","125壳架  125A/3/带辅助报警触头(热磁、电动机保护)","台"]
[{"$nulls":5},"塑壳断路器","125壳架  63A/3/带辅助报警触头(电子式)","台"]
[{"$nulls":5},"塑壳断路器","125壳架 125A/3/带辅助触头(隔离型)","台"]
[48,"标段四十八","电池、蓄电池架",null,null,"电池","2V,800Ah（带阻燃，配连接排）","只"]
[{"$nulls":5},"电池","2V,500Ah（带阻燃，配连接排）","只"]
[{"$nulls":5},"电池","2V,400Ah（带阻燃，配连接排）","只"]
[{"$nulls":5},"电池","2V,200Ah（带阻燃，配连接排）","只"]
[{"$nulls":5},"电池","12V,100Ah（带阻燃，配连接软线）","只"]
[{"$nulls":5},"电池","12V,150Ah（带阻燃，配连接软线）","只"]
[{"$nulls":5},"电池","12V,40Ah","只"]
[{"$nulls":5},"电池","12V,24Ah","只"]
[{"$nulls":5},"电池","12V,20Ah","只"]
[{"$nulls":5},"蓄电池架","两层两列，尺寸为：5388mmx480mm，每套配4个接线箱（500Ah）","套"]
[{"$nulls":5},"蓄电池架","三层两列，尺寸为：1890mmx410mm，每套配2个接线箱（400Ah）","套"]
[{"$nulls":5},"蓄电池架","两层四列，尺寸为：2340mmx864mm，每套配4个接线箱（400Ah）","套"]
[{"$nulls":5},"蓄电池架","三层两列，尺寸为：3780mmx700mm，每套配4个接线箱（800Ah）","套"]
[{"$nulls":5},"蓄电池架","三层两列，尺寸为：3780mmx480mm，每套配4个接线箱（500Ah）","套"]
[{"$nulls":5},"蓄电池架","三层两列，尺寸为：3780mmx410mm，每套配4个接线箱（400Ah）","套"]
[49,"标段四十九","交直流电源系统用模块、监控系统、UPS","包49-1","模块&监控","高频开关电源模块","AC380V转DC220V40A","只"]
[{"$nulls":5},"高频开关电源模块","AC380V转DC220V30A  ","只"]
[{"$nulls":5},"高频开关电源模块","AC380V转DC220V20A  ","只"]
[{"$nulls":5},"高频开关电源模块","AC380V转DC220V10A  ","只"]
[{"$nulls":5},"高频开关电源模块","AC380V转DC110V10A  ","只"]
[{"$nulls":5},"高频开关电源模块","AC220V转DC110V 10A","只"]
[{"$nulls":5},"高频开关电源模块","AC220V转DC110V 5A","只"]
[{"$nulls":5},"通信电源模块","DC220V转DC48V50A","只"]
[{"$nulls":5},"通信电源模块","DC220V转DC48V30A","只"]
[{"$nulls":5},"通讯电源模块","DC220V转DC48V20A  ","只"]
[{"$nulls":5},"通信电源模块","DC110V转DC48V50A","只"]
[{"$nulls":5},"通信电源模块","DC110V转DC48V30A","只"]
[{"$nulls":5},"通讯电源模块","DC110V转DC48V20A  ","只"]
[{"$nulls":5},"通讯电源模块","DC110V转DC24V30A  ","只"]
[{"$nulls":5},"24V开关电源模块","150W","只"]
[{"$nulls":5},"交流测控","交流测控模块","只"]
[{"$nulls":5},"交流监控模块","交流监控（含24V电源1个、接口转换器1个）","只"]
[{"$nulls":5},"备自投","BZT  3路三相交流电流测量接口;3路三相交流电压测量接口，可控制交流互投;","只"]
[{"$nulls":5},"备自投监控","JLNB（带接口转换器2个和24V电源模块1个）","只"]
[{"$nulls":5},"直流监控模块","直流监控(含霍尔传感器200A)直流电源监控，七寸触摸屏,带8路开入,3路开出,1路综合故障告警(一组常开和1组常闭点,可选择成为综合故障或者监控故障),自带采集:一组电池电压,一路合母电压,一路控母电压,一路交流电压,一组电池电流,充电模块数据，UPS数据，逆变器数据，DCDC电源数据；通讯有三路485COM口,一路CAN通讯口,带闭码对时,工作电源88V-286VDC","只"]
[{"$nulls":5},"综合测量","采集交流电压、电池电压、控母电压、合母电压、控母电流、电池电流、温度及开关量输入和开关量输出，并通过RS485接口将数据上传到监控主机","只"]
[{"$nulls":5},"绝缘监测主机","绝缘监测主机","只"]
[{"$nulls":5},"通讯电源监控模块","通讯电源监控模块","只"]
[{"$nulls":5},"总监控","ZJK（含24V电源模块1个、接口转换器3个）10寸彩色触摸屏，主要作为大型系统的总监控使用，可以搭配子监控，作为系统的总监控装置,可以显示每一个子系统的信息","只"]
[{"$nulls":5},"总监控","总监控（含24V电源1个、接口转换器1个）总监控,七寸触摸屏,带8路开入，3路开出，1路综合故障告警(一组常开和1组常闭点，可选择成为综合故障，或者监控故障),可以带3个直流电源监控,2个绝缘检测主机,2个交流监控,2个DCDC电源监控,带闭码对时,工作电源88V-286VDC","只"]
[{"$nulls":5},"直流监控器","直流监控（DC110V系统）适用居配工程","只"]
[{"$nulls":5},"工控机","61850A（含通讯接口、电源，适用110KV变电站一体化电源）","只"]
[{"$nulls":5},"工控机","61850B（含通讯接口、电源，适用220KV及以上变电站一体化电源）","只"]
[{"$nulls":5},"开关量模块","32路开关量","只"]
[{"$nulls":5},"开关量模块","64路开关量","只"]
[{"$nulls":5},"支路检测模块","ZLJC-64单台模块可以同时采集开关量状态告警和支路绝缘共64路,工作电源88V-286VDC","只"]
[{"$nulls":5},"支路检测模块","ZLJC-32单台模块可以同时采集开关量状态告警和支路绝缘共64路,工作电源88V-286VDC","只"]
[{"$nulls":5},"B码对时盒","BMDS 2.0","只"]
[{"$nulls":5},"电池巡检仪","电池巡检12V18节 采集电池单体电压及环境温度，小数点后三位精度","只"]
[{"$nulls":5},"电池巡检仪","电池巡检2V55节 采集电池单体电压及环境温度，小数点后三位精度","只"]
[{"$nulls":3},"包49-2","UPS类","UPS模块","单相5kVA变压器内置 （DC220V）","只"]
[{"$nulls":5},"UPS模块","单相8kVA变压器内置  （DC220V）","只"]
[{"$nulls":5},"UPS模块","三相10kVA变压器外置  （DC220V）","只"]
[{"$nulls":5},"UPS模块","三相15kVA变压器外置  （DC220V）","只"]
[{"$nulls":5},"UPS模块","单相5kVA变压器内置 （DC110V）","只"]
[{"$nulls":5},"UPS模块","单相8kVA变压器内置  （DC110V）","只"]
[{"$nulls":5},"UPS模块","三相10kVA变压器外置  （DC110V）","只"]
[{"$nulls":5},"UPS模块","三相15kVA变压器外置  （DC110V）","只"]
[{"$nulls":5},"逆变模块","逆变模块5kVA","只"]
[{"$nulls":5},"旁路隔离变压器","AC220V/AC220V 5KVA  ","只"]
[{"$nulls":5},"旁路隔离变压器","AC220V/AC220V 8KVA  ","只"]
[{"$nulls":5},"旁路隔离变压器","AC220V/AC220V 10KVA  ","只"]
[{"$nulls":5},"旁路隔离变压器","AC220V/AC220V 15KVA  ","只"]
[{"$nulls":3},"包49-3","传感器类","漏电流传感器","10mA  微断用","只"]
[{"$nulls":5},"漏电流传感器","10mA  塑壳用","只"]
[{"$nulls":5},"霍尔传感器","300A","只"]
[{"$nulls":5},"霍尔传感器","400A","只"]
[{"$nulls":5},"霍尔传感器","600A","只"]
[{"$nulls":3},"包49-4","硅链类","降压硅链（带斩波）","DZB/5A-20A20V-DC110V    直流110V系统  5级调节","只"]
[{"$nulls":5},"降压硅链","DJA/5A-10A20V-DC110V    直流110V系统   5级调节","只"]
[{"$nulls":5},"降压硅链","DJA/5A-20A20V-DC110V    直流110V系统   5级调节","只"]
[{"$nulls":5},"降压硅链","DJA/5A-30A20V-DC110V    直流110V系统   5级调节","只"]
[{"$nulls":5},"降压硅链","DJA/5A-10A35V-DC220V    直流220V系统   7级调节","只"]
[{"$nulls":5},"降压硅链","DJA/5A-20A35V-DC220V    直流220V系统   7级调节","只"]
[{"$nulls":5},"降压硅链","DJA/5A-30A35V-DC220V    直流220V系统   7级调节","只"]
[{"$nulls":5},"降压硅链","DJA/5A-40A35V-DC220V    直流220V系统   7级调节","只"]