{"text_format":"3","workbook":"xlsx","n_sheets":5,"sheets":["本部检验设备","CNAS实验室设备","实验室设备2","工程一部设备","安全工器具台账"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"本部检验设备","index":0,"n_rows":86,"n_cols":14,"rows_kept":86,"merged":[[0,0,0,9],[1,0,1,9]]}
["扬州北辰电气集团有限公司\n监视、测量装置台帐\n"]
["YZBC/QD7.6-01"]
["序号","设备名称","型号/规格","测量范围","准确度","使用部门","出厂编号","制造厂","启用日期","备注"]
[1,"局部放电测试仪","TCD-9302","6PF～250μF",null,"质量管理部","BY002","扬州唐城",2006.4]
[2,"电池型绝缘电阻表","MODEL-3121A","2500V/100000MΩ",null,"质量管理部","W0291256","日本共立",2007.2]
[3,"微水仪","GSM-05",null,null,"售后服务部",271398,"常州集贤",2007.9]
[4,"回路电阻测试仪","PCIμΩ/3","0～1999μΩ","0.5级","质量管理部",8114,"上海沪西电器",2009.4]
[5,"绝缘电阻测试仪","KEW 3121A","2500V/100000MΩ",null,"质量管理部","W0285841","共立仪器",2010.1]
[6,"开关机械特性测试仪","GKC-98H8",null,null,"工程一部",100231,"珠海英之泰电气",2010.1]
[7,"接地电阻测试仪","YD2668-4B",null,null,"质量管理部","68.48.2090","常州扬子电子",2010.3]
[8,"耐压测试仪","YD2673","0～5000V",null,"质量管理部",2673.2846,"常州扬子电子",2010.3]
[9,"SF6气体检漏仪","Q200",null,null,"质量管理部",2002130,"美国USON",2011.1]
[10,"继电器综合试验装置","KVA-5",null,null,"质量管理部","A1211160028","上海舒佳电气"]
[11,"高压试验设备","YDT-5KVA/100KV",null,null,"工程一部",83489,"上海源佳通",2012.1]
[12,"保护电路连接有效性测试仪","BH-1","0-120mmΩ",null,"质量管理部","ZJ030","苏州友邦"]
[13,"耐压测试仪","YX2670AC","0-10kV","0.5级","质量管理部",3660,"江苏一星科学仪器厂",2013.4]
[14,"绝缘电阻测试仪","YX2674","25V-1000V","0.5级","质量管理部",3626,"江苏一星科学仪器厂",2013.4,{"$nulls":4},"                                                                                                                                                                                                                                                                                                                                                        "]
[15,"数显卡尺","0-150mm","0-150mm","0.01mm","质量管理部","C1303255616","桂林广陆数字测控股份有限公司",2013.5]
[16,"数显卡尺","0-300mm","0-300mm","0.01mm","质量管理部","C1207245559","桂林广陆数字测控股份有限公司",2013.5]
[17,"数字万用表","FLUKE17B",null,null,"生产管理部","27161705WS","FLUKE",2014.9]
[18,"智能断路器剩余电流特性测试台","定制","380V/50HZ/15KVA/10~600A/0~5V","0.5级","生产管理部",1408002,"松乐自动化",2014.9]
[19,"大电流发生器","YSB895-1000A","0~1000A",null,"质量管理部",15032102,"扬州市双宝电力设备",2015.3]
[20,"继电保护试验箱","YSB813","0-2500.0v/0-500mA/0-10.00A","0.5级","质量管理部",1503206,"扬州市双宝电力设备",2015.3]
[21,"互感器综合测试仪","YSB843",null,null,"工程一部",15032101,"扬州市双宝电力设备",2015.3]
[22,"手持式合金分析仪","Genius5000 XRF",null,null,"工程一部","100500002-00142A","天瑞仪器股份有限公司",2015.3]
[23,"覆层测厚仪","TT210",null,null,"质量管理部",29787000010,"北京时代之峰科技有限公司",2015.4]
[24,"三倍频电源发生器","HXSF",null,null,"质量管理部",150522,"扬州鸿熙电气有限公司",2015.4]
[25,"电力专用油色谱分析仪","GWC-9560",null,null,"质量管理部",182091,"武汉华威电气有限公司"]
[26,"油微量水份测试仪","GWS-106",null,null,"质量管理部",31400025,"武汉华威电气有限公司"]
[27,"精密油介损测试仪","GW6100",null,null,"质量管理部",31400026,"武汉华威电气有限公司"]
[28,"超声波测厚仪","TIME®2430",null,null,"质量管理部",5059803,"北京时代之峰科技有限公司"]
[29,"直流电阻测试仪","ZGY-III",null,null,"质量管理部",1609007,"扬州久源电气科技有限公司"]
[30,"变比测试仪","YSB825",null,null,"工程一部",1609008,"扬州久源电气科技有限公司"]
[31,"油耐压测试仪","YSB861",null,null,"质量管理部",1609009,"扬州久源电气科技有限公司"]
[32,"变压器综合试验台","YSB821",null,null,"质量管理部",1609018,"扬州久源电气科技有限公司"]
[33,"功率分析仪","AWS2103",null,null,"质量管理部",140315225,"肈慶爱特精密测量科技有限公司"]
[34,"双踪示波器","CA9020A",null,null,"质量管理部","09JG1452","扬中科泰电子"]
[35,"负载箱","HB-DC11K/0.22D","220/110V  1-50A 11kW",null,"质量管理部",1011036,"上海汉标电子"]
[36,"电源控制台","DYT-I",null,null,"质量管理部",201001,"扬州北辰"]
[37,"回路电阻测试仪","HLY-IV",null,null,"质量管理部","A0903100102","上海舒佳电气"]
[38,"开关机械特性测试仪","SWT-Ⅱ",null,null,"质量管理部","S18146","西安博能电力"]
[39,"回路电阻测试仪","WHL-100",null,null,"开关事业部","B041","南京沃派科技有限公司"]
[40,"互感器变比极性测试仪","WPBJ-2",null,null,"质量管理部","002718","南京沃派科技有限公司",2019.2]
[41,"游标卡尺",null,"0--150mm",null,"质量管理部",4391,"哈尔滨量具"]
[42,"深度尺",null,"0-200mm",null,"质量管理部",3034,"哈尔滨量具"]
[43,"深度尺",null,"0-200mm",null,"质量管理部",3154,"哈尔滨量具"]
[44,"工频耐压试验系统","JTKZ-5KVA/50KV/100KV",null,null,"质量管理部",19042162,"上海佳特高压电气",2019.4]
[45,"超声波测厚仪","27MG-M-I-ZH",null,null,"质量管理部",190739609,"OLYMPUS/奥林巴斯",2019]
[46,"数显千分尺",null,"0-25mm","0.001mm","质量管理部","B49620","桂林广陆数字测控股份有限公司"]
[48,"冲击电压发生器(1、冲击电压发生器本体YXYCJ-10KJ/400KV 2、弱阻尼电容分压器RZF-400KV 3、直流充电装置ZCD±100KV 4、冲击电压试验控制台YXY-CJ60)","CJDY-400/CJ-II",null,null,"开关事业部","180128-1","江苏新亚高压测试设备有限公司"]
[49,"开关机械特性测试仪","KWP-300",null,null,"开关事业部","B121","南京沃派科技有限公司"]
[50,"钳型电流表","FLUKE319",null,null,"质量管理部","36090135WS","FLUKE"]
[51,"SF6定量捡漏仪","WP-Y-85",null,null,"开关事业部",18114,"上海科石科技发展有限公司"]
[52,"数字电导率仪","PZ 60A",null,null,"质量管理部",14168641,"东莞市展鹏电子仪器有限公司"]
[53,"高低压开关通电试验台","TDSY-3","AC：380V 三相四线 50Hz",null,"开关事业部","01903011","南京沃派科技有限公司",2019.3]
[54,"接地电阻测试仪","HC2571","0-120mmΩ/0.1mΩ",null,"质量管理部","202011469","南京沃派科技有限公司",2020.12]
[55,"直流高压发生器","HCZGF-120kv","DC:120Kv/3mA",null,"质量事业部","202011466","武汉汉测",2020.12]
[56,"三相继电保护测试仪","HCTB","三相电压电流个2组",null,"质量事业部",202011468,"武汉汉测",2020.12]
[57,"绝缘电阻测试仪","HC2305","DC:0-5000V 200GΩ ",null,"质量事业部",75190073,"武汉汉测",2020.12]
[58,"变频串联谐振(1、电容分压器FRC-1000PF/80Kv 2、变频串联谐振试验成套装置HCXZ-7.5KVA/75KV/1A 3、高压电抗器DK-25KVA/25KV(3只))4、激励变压器JL-4KVA",null,"75KvA/75Kv/1A",null,"质量事业部",null,"武汉汉测",2020.12]
[59,"数字万用表","FLUKE 17B+",null,null,"质量事业部","48911719WS","FLUKE"]
[60,"钳形电流表","FLUKE 36","0-1000A",null,"质量事业部",78214548,"FLUKE"]
[61,"充放电试验台","DC104","输出电压：0~1200VDC",null,"质量事业部",20214646,"杭州得诚电力科技股份有限公司",2021.1]
[62,"绝缘电阻测试仪","KEW3441","0-1000V",null,"质量事业部","0214067","日本共立",2021.11]
[63,"三相泄漏电流测试仪","WB2675S",null,null,"全电厨房","WB2675S211106","杭州威博科技有限公司"]
[64,"三相智能电参数测量仪","PZ-9930",null,null,"全电厨房","20102261","佛山华之科技有有限公司"]
[65,"直流电源","DC 0-220V",null,null,"质量事业部","B067-B070","南京金宇星拓","4台"]
[66,"互感器综合测试仪"," FA-2000",null,null,"质量事业部","B071","南京沃派科技有限公司"]
[67,"光泽度仪","MODEL WG60A",{"$nulls":3},"60A150696"]
[68,"涂层测试仪","DF-156",{"$nulls":3},"12107472","深圳华盛昌机械"]
[69,"真空氦漏孔","TL4-6",null,null,"开关事业部","90001530388","德国英福康"]
[70,"电导率测试仪","PZ60A",null,null,"质量事业部","1416861","德国英福康","2020.8.24"]
[71,"智能断路器老化控制台","定制",null,null,"生产管理部",1408003,"松乐自动化",2014.9]
[72,"智能断路器63-630型标桩长延时控制台","定制",null,null,"生产管理部",2014083001,"松乐自动化",2014.9]
[73,"噪声计","TES-1357",null,null,"质量事业部",151100791,"泰仕电子工业股份有限公司",null,"031400032"]
[74,"无局放试验变压器","HXQD-30KVA120KV",null,null,"质量管理部",150520,"鸿熙电气有限公司",2015.5,"031400020"]
[75,"电子吊钓称","OCS-EW-5t"," ","1kg","生产管理部",1609108,"宁波依托力称重设备有限公司",2016.12]
[76,"电子台秤","XK3190-A23P","30kg","Ⅲ级","生产管理部",1503054639,"上海耀华称重有限公司",2016.12]
[77,"电子地上衡","SCS-3","20-3000kg",null,"生产管理部",1610201,"常州力诺电子衡器有限公司",2016.12]
[78,"回路电阻测试仪","WHL-100","0～19999μΩ",0.5,"质量管理部","H2212","南京沃派科技有限公司",2022.4]
[79,"高压分压器（数字高压表）","FRC-150","1800MΩ","AC:10.% DC:015%","质量管理部",2203266,"南京沃派科技有限公司",2022.4]
[80,"通电试验台","DTSY-5","三相0-600v     ",null,"开关事业部",220431,"南京沃派科技有限公司",2022.5]
[81,"无功补偿柜噪音测试平衡负载系统","STLS-420","容量60KVA",null,"质量管理部","ZS20220435","国科元玮电气科技（苏州）有限公司",2022.5]
[82,"钢卷尺","GW-366-5","3M",null,"质量管理部",11533,"长城",2022.9]
[83,"数显外径千分尺","0-25mm",null,"0.001mm","质量管理部","D31511","桂林广陆数字测控股份有限公司"]
[84,"数显外径千分尺","0-25mm",null,"0.001mm","质量管理部","D31504","桂林广陆数字测控股份有限公司"]

{"sheet":"CNAS实验室设备","index":1,"n_rows":48,"n_cols":7,"rows_kept":48,"merged":[[0,0,0,6],[5,0,7,0],[5,1,7,1],[5,2,7,2],[37,0,39,0],[37,1,39,1],[37,2,39,2],[37,3,39,3],[37,4,39,4],[37,6,39,6]]}
["检测仪器设备检定校准参数要求表"]
["表单编号：BCL 230-02-A0"]
["本所编号","设备名称","型号规格","测量范围","准确度","检定校准参数检测点及精度要求","生产厂家"]
["C011","钢卷尺","GW366-5","3m",null,"量程：1m，2m, 3m  精度：±0.2mm","浙江长城"]
["2665D-859","工频耐压试验仪","YD2665D","0-2.5kv/5kv","±3%","电压AC：1、1.89、2.5、4、5kV， 精度：±3%","常州扬子电子"]
["68.48.2090","接地电阻测试仪","YD2668-4B","5-10A:0-0.5Ω","±5%","报警预置值：100mΩ， 精度：±1%\n电流：10A、25A，精度：±3%\n","常州扬子电子"]
[{"$nulls":3},"10-20A:0-0.3Ω","±3%"]
[{"$nulls":3},"20-30A:0-0.2Ω","±3%"]
[201406,"游标卡尺","PD151","150mm","0.02mm","量程：5、10、12、14、20、30、50、100、150mm，准确度：0.02mm","上海宝工工具有限公司"]
["BND2014120203","爬电距离卡",null,"1.0-8.0mm","±0.03mm","每个尺寸检定尺寸：1.0mm,1.5mm,2.0mm,2.5mm,3.0mm,4.0mm,6.0mm,8.0mm；精度±0.03mm","深圳联合博纳精密仪器"]
["HT20141205A1","试验探针","HT-I04","￠1mm",null,"直径：1mm；   精度要求：＋0.05 mm         长度：100mm； 精度要求：±0.2mm","广州泓通检测设备有限公司"]
["HT20141205A2","试验探针","HT-I03","￠2.5mm",null,"直径：2.5mm； 精度要求：＋0.05 mm                 长度：100mm   精度要求：±0.2mm","广州泓通检测设备有限公司"]
["XMZ-141201","多路温度巡回检测仪","XMZ-J1638",null,null,"各通道校准：（-30、100、200、300）℃","余姚长江温度仪表厂"]
["XMZ-141202","多路温度巡回检测仪","XMZ-J1638",null,null,"各通道校准：（-30、100、200、300）℃","余姚长江温度仪表厂"]
["BCT133","热电偶","K型","0～450℃",null,"温度：（70、100、125）℃，精度±2.5℃"]
["BCT101～108","铂电阻","Pt100",null,null,"检测点：（-10、0、25、40、70、100、125）℃"]
["HT20141205A3","钢球","HT-I05","￠50mm",null,"直径：50mm；  精度要求：＋0.05 mm","广州泓通检测设备有限公司"]
[1412042,"关节试验指","FZ-1101A","￠12mm",null,"挡盘：圆弧直径50±0.2mm，宽度20±0.2mm                      直径：12mm；  精度要求：＋0.05 mm      长度：80mm    精度要求：±0.3mm       ","东莞瀚阳电子仪器有限公司"]
["2414I05024","指针式推拉力测试仪","SN-50","0-50N","±1%FS","拉压力：1±0.1，3±0.3，30±3，50±5N；","温州山度仪器有限公司"]
[2014121,"滴水试验装置","DL-B","IPX1/IPX2",null,"检定流量计（100,300,500）L/h ±5%","江苏艾默生试验仪器"]
[2014122,"摆管淋雨试验装置","BL-16","IPX3/IPX4",null,"检定流量计（400,600,900）L/h ±5%","江苏艾默生试验仪器"]
["2014121-1","玻璃转子流量计","LZB-25"]
["2014121-2","玻璃转子流量计","LZB-25"]
[2014117,"盐雾试验箱","YWXQ-750/B",null,null,"温度：35℃，精度：±2℃\n盐雾沉降量：1ml（h•80c㎡）＜G＜2ml（h•80c㎡）\n","江苏艾默生试验仪器"]
[2014118,"高低温湿热试验箱","GDJS-08","–40-150℃/30-98%",null,"温度：校准﹣15、0、25、40、55、70、100、125，精度±2℃；温湿度：校准（40℃、95%）（25℃、90%）（55℃、95%），精度：(≥75%RH,±3%)(＜75%RH,±5%)；交变速率：1℃/min，±5%","江苏艾默生试验仪器"]
[20150422,"秒表","PC2810",null,"0.01s",null,"深圳市惠波工贸有限公司"]
[201401119,"球压试验设备","QY-2","20N",null,"直径5mm,±0.1mm；压力20N，±1N","武汉信鼎科技有限公司"]
["                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ","电子天平","T500","500g","0.1g","检定50、200、500g三点，误差±0.1g","常熟双杰测试仪器厂"]
[213,"电导率仪","DDS-11A","0-2×105μS/cm","1.0级","计示值:电子单元重复性、电子单元引用误差、电导池常数示值误差，最大允许误差分别为 1.3%FS、±4%FS、±0.02cm-1；仪器示值：温度示值误差、仪器引用误差、仪器重复性，最大允许误差分别为±2℃、±4.5%FS、0.26%FS；准确度：1.0级","上海雷磁创益仪器仪表"]
[1412055,"水平垂直燃烧试验仪","XD550",null,null,"计时：30s、60s、100s，精度：±0.5s；计数：10、100，精度：±1","武汉信鼎科技有限公司"]
["BCT-01","温湿度计","WS-B2","机械式：–20-50℃",null,"温度：-10℃、15℃、25℃、35℃、45℃； 精度：±0.5℃；湿度：30%、45%、55%、65%、75%、90%RH； 精度：±5%","上海天宇科技仪表有限公司"]
["BCT-02～06","温湿度计（5个）",8813,"电子式：–40-60℃",null,"温度：-10℃、15℃、25℃、35℃、45℃； 精度：±1℃；湿度：30%、45%、55%、65%、75%、90%RH； 精度：±5%","得力集团有限公司"]
["ZC140835","微机控制弹簧拉压试验机","ZCTL-W500N","0～500N","1级","试验力:100N,200N,300N,400N,500N， 精度：±1% ","中创工业测试系统有限公司"]
[14090213,"空盒气压表","DYM3","800-1064hPa",null,"气压：取6个点气压测量， 精度：±1%","宁波姜山玻璃仪器仪表厂"]
["5A14D01280","推拉力测试仪","SH-1K","1000N",null,"推拉力：5、10、50、100、500、1000N， 精度：±1%","温州山度仪器有限公司"]
["600710N0015120071","PH计","PHS-3E","pH：0.00～14.00pH mV:0～±1999mV    温度：0～99.9℃","0.01级","取3个点检定，其中一个7.0，最大允差±0.02pH","上海雷磁创益仪器仪表"]
[20150126,"读数显微镜","JC10","20倍   0～6mm","0.01mm","刻度值：（0、1、2、3、4.8）mm，准确度0.01mm","华银仪器设备有限公司"]
[1412054,"灼热丝试验仪","XD5101A",null,null,"温度：（550、650、750、850、960）℃ ","武汉信鼎科技有限公司"]
[{"$nulls":5},"小车行进速度：10mm～25mm/s"]
[{"$nulls":5},"灼热丝顶部冲击值（压力）：1±0.2N"]
[19121901,"三相大电流发生器","JTSDL-4000A/10","0-4000A","0.01级","A、B、C相分别设定250A、400A、630A、800A、1600A、2500A，最大允许误差±3%","上海佳特高压电气设备有限公司"]
[19121802,"局放试验仪（成套）","JFD-2010",{"$nulls":3},"上海佳特高压电气设备有限公司"]
[20082335,"大电流调节负载箱","JTL-800A","0-800A",null,"电流100A、200A、300A、400A、500A、600A、700A、800A，最大允许误差±3%","上海佳特高压电气设备有限公司"]
[19121903,"负载调节柜","JTTL-400","0-400A",null,"电流50A、100A、150A、200A、250A、300A、350A、400A，最大允许误差±3%","上海佳特高压电气设备有限公司"]
[19121904,"负载调节柜","JTTL-800","0-800A",null,"电流100A、200A、300A、400A、500A、600A、700A、800A，最大允许误差±3%","上海佳特高压电气设备有限公司"]
["0609205002873","温度记录仪","TP1000",null,null,"温度测量通道20个点，最大允许误差±0.3℃","上海佳特高压电气设备有限公司"]
[19121902,"无纸记录仪（热电偶试验箱）","GX20-IC",null,null,"温度测量通道20个点，最大允许误差±0.3℃","上海佳特高压电气设备有限公司"]
[19121801,"局放房屏蔽效果",{"$nulls":4},"上海佳特高压电气设备有限公司"]

{"sheet":"实验室设备2","index":2,"n_rows":24,"n_cols":6,"rows_kept":24,"merged":[[0,0,0,5],[1,0,1,5]]}
["检测站设备台账\n"]
["YZBC/QD7.6-01"]
["序号","设备名称","型号/规格","出厂编号","制造厂","备注"]
[1,"微机型继电保护测试系统","PL461",140191101,"博电"]
[2,"静电放电发生器","ESD20H","ES0101955","苏州泰斯特电子科技有限公司"]
[3,"交流采样送变器校验仪","PM205AM",3271911001,"博电"]
[4,"电子互感器校验仪","PET100N",508191101,"博电"]
[5,"群脉冲发生器","EFT-4003G","ES0201919","3ctest/泰斯特"]
[6,"全自动雷击浪涌发生器","CWS600G",1912110,"3ctest/泰斯特"]
[7,"浪涌耦合/去藕网络","CND405M40","ES2711919","3ctest/泰斯特"]
[8,"沙尘试验箱","YSCX-010","YS19110401XL-02","上海毅硕实验仪器厂"]
[9,"三相功率源/电源功放","PAV250Bi",845190402,"博电"]
[10,"三相标准表","M3005","M3005190402","博电"]
[11,"精密电流互感器","NAHL-1000A","NA201861374","南澳电气（武汉）有限公司"]
[12,"电流互感器","NAHFG-5000A/5A/1A","NA1911605","南澳电气（武汉）有限公司"]
[13,"直流电子负载","CH9720CU","LO-9B-13449","BEICH/贝奇"]
[14,"耦合夹","CCC100","CCC19092895","3ctest/泰斯特"]
[15,"耦合去耦网络","SPN3816T",1912120,"4ctest/泰斯特"]
[16,"高低温交变湿热试验箱","YSGJS-010B","YS19110401","上海毅硕实验仪器厂"]
[17,"功率计","CH2802","PO-9C-1102","BEICH/贝奇"]
[18,"交流调压电源","STG-2000W","TY001","浙江广伏"]
[19,"直流电压源","6005  60v  5A","CH1906D600520","艾维泰科"]
[20,"数字式摇表/绝缘电阻测试仪","3005A","E8248465","克列茨"]
[21,"数字式万用表","34461A","MY59011609","KEYSIGHT"]

{"sheet":"工程一部设备","index":3,"n_rows":54,"n_cols":6,"rows_kept":54,"merged":[[0,0,0,5],[1,0,1,5]]}
["工程服务中心一部设备台账\n"]
["YZBC/QD7.6-01"]
["序号","设备名称","型号/规格","使用部门","出厂编号","制造厂"]
[1,"接触调压器","TSGC-15KVA","工程服务中心一部","01/02","浙江人民电器有限公司"]
[2,"高压试验设备","YDT-5KVA/100KV","工程服务中心一部",83489,"上海源佳通电气有限公司"]
[3,"变频电源","RT-15KW/220/380V","工程服务中心一部","0171227002B、0171227001B","咸亨国际电气制造有限公司"]
[4,"电容分压器","FRC-30KV/1500PF","工程服务中心一部","0171227001D/0171227002D","咸亨国际电气制造有限公司"]
[5,"补偿电容器","BC-30KV/5000PF","工程服务中心一部","0171227001R/0171227002R","咸亨国际电气制造有限公司"]
[6,"激励变压器","RTE-7.5KVA/1.5KV/0.4KV","工程服务中心一部","0171227001J1、J2","咸亨国际电气制造有限公司"]
[7,"激励变压器","RTE-7.5KVA/1.5KV/0.4KV","工程服务中心一部","0171227002J1、J2","咸亨国际电气制造有限公司"]
[8,"高压电抗器","RTE-75KVA/30KV","工程服务中心一部","0171227001K1-K4","咸亨国际电气制造有限公司"]
[9,"高压电抗器","RTE-75KVA/30KV","工程服务中心一部","0171227002K1-K4","咸亨国际电气制造有限公司"]
[10,"电缆测长仪","WL20","工程服务中心一部","X0161112021","咸亨国际电气制造有限公司"]
[11,"高压电阻绝缘测试仪","S325U/5000V","工程服务中心一部","200005362                   200005361","咸亨国际电气制造有限公司"]
[12,"变压器容量特性测试仪","HXOT325L","工程服务中心一部",8101638098,"咸亨国际电气制造有限公司"]
[13,"直流电阻测试仪","ZGY-III","工程服务中心一部",1609007,"扬州久源电气科技有限公司"]
[14,"全自动变比测试仪","YSB825","工程服务中心一部",1609008,"扬州久源电气科技有限公司"]
[15,"高压开关综合测试仪","GKC-98H8","工程服务中心一部",100231,"珠海英之泰电气"]
[16,"阻容分压器","RCVD-100KV","工程服务中心一部",20161100,"上海蓝波高电"]
[17,"三相交直流指示仪检测装置","DK-56B1","工程服务中心一部","301B-1011B-0483 /             301B-1011B-0481         ","南京丹迪克科技开发有限公司"]
[18,"变压器变比测试仪","HXOT263E","工程服务中心一部",7102541032,"咸亨国际电气制造有限公司"]
[19,"变压器空负载损耗测试仪","HCSH-II","工程服务中心一部",10262,"武汉汉测电气有限公司"]
[20,"变压器空负载测试仪","YSB821","工程服务中心一部",1609018,"扬州久源电气科技有限公司"]
[21,"手持式分析仪","DELTADPO2000","工程服务中心一部",543742,"奥林巴斯有限公司"]
[22,"工频耐压试验箱","     ","工程服务中心一部",20021271,"上海佳特高压电气有限公司"]
[23,"互感器综合特性测试仪","HXT472E","工程服务中心一部",7102360024,"咸亨国际电气制造有限公司"]
[24,"电缆测长仪","WL20","工程服务中心一部","T020171212001","咸亨国际电气制造有限公司"]
[25,"变压器直流电阻测试仪","DCR-10","工程服务中心一部",7102433005,"咸亨国际电气制造有限公司"]
[26,"汽油发电机","ATH-3160","工程服务中心一部",null,"久保田"]
[27,"直流电阻测试仪","WP5854-10","工程服务中心一部","01182537","南京沃派科技有限公司"]
[28,"数显卡尺","0-150mm","工程服务中心一部","KI6F155982","桂林广陆数字测控股份有限公司"]
[29,"数显卡尺","0-150mm","工程服务中心一部","KI6F155969","桂林广陆数字测控股份有限公司"]
[30,"数显外径千分尺","0-25mm","工程服务中心一部","T67680","桂林广陆数字测控股份有限公司"]
[31,"数显外径千分尺","0-25mm","工程服务中心一部","T67695","桂林广陆数字测控股份有限公司"]
[32,"数显卡尺","0-150mm","工程服务中心一部","KI7C315115","桂林广陆数字测控股份有限公司"]
[33,"变压器空负载特性分析仪","WP2810A","工程服务中心一部",186160,"南京沃派科技有限公司"]
[34,"互感器变比极性测试仪","WPBJ-2","工程服务中心一部","0002737","南京沃派科技有限公司"]
[35,"互感器测试仪","FA-2000","工程服务中心一部",null,"南京沃派科技有限公司"]
[36,"直流电阻测试仪","ZDC-20A","工程服务中心一部","011903280629","南京沃派科技有限公司"]
[37,"互感器综合测试仪","YSB843","工程服务中心一部",15032101,"扬州双宝电力设备有限公司"]
[38,"电缆测长仪","WL20","工程服务中心一部","XO180817003","咸亨国际电气制造有限公司"]
[39,"合金分析仪","Element-s","工程服务中心一部","087614","奥林巴斯有限公司"]
[40,"变压器容量空负载测试仪","HCRL-II","工程服务中心一部","H0089","武汉汉测电气有限公司"]
[41,"直流电阻测试仪","HCZZ-20A","工程服务中心一部","H0087/H0088","武汉汉测电气有限公司"]
[42,"互感器综合测试仪","HCVA-III","工程服务中心一部","H0090","武汉汉测电气有限公司"]
[43,"调压器","TSGC2-15KVA","工程服务中心一部","03","温州卓伟电子科技有限公司"]
[44,"电缆测长仪","WL20","工程服务中心一部","XO201206018","咸亨国际电气制造有限公司"]
[45,"能量色散X荧光光谱仪及软件","XP30","工程服务中心一部",null,"苏州"]
[46,"便携式局放检测仪","HPS003A","工程服务中心一部",9211011071,"浙江红谱有限公司"]
[47,"综合带电检测仪","PDS-T95","工程服务中心一部","2FC79D21030000F7","华乘电气科技股份有限公司"]
[48,"红外热成像仪","HT-1R1-320","工程服务中心一部","21S2K992005","苏州华天国科电力"]
[49,"互感器综合测试仪","HCVA-III","工程服务中心一部","010211","武汉汉测电气有限公司"]
[50,"变压器容量空载测试仪","HCRL-II","工程服务中心一部","HC01026","武汉汉测电气有限公司"]
[51,"直流电阻测试仪","HCZZ-20","工程服务中心一部","HC11026","武汉汉测电气有限公司"]

{"sheet":"安全工器具台账","index":4,"n_rows":44,"n_cols":9,"rows_kept":44,"merged":[[0,0,0,8]]}
["施工机具、安全工器具台账"]
["序号","外包单位名称","机具名称","机具类别（施工机具/安全工器具）","生产日期","检验证书编号","检验单位","有效期","备注"]
[1,"扬州北辰电气集团有限公司","绝缘手套","安全工器具","2019-12-01",{"$nulls":3},"工程一部"]
[2,"扬州北辰电气集团有限公司","绝缘手套","安全工器具","2019-12-01",{"$nulls":3},"工程一部"]
[3,"扬州北辰电气集团有限公司","绝缘手套","安全工器具","2019-12-01",{"$nulls":3},"工程一部"]
[4,"扬州北辰电气集团有限公司","绝缘手套","安全工器具","2019-12-01",{"$nulls":3},"工程一部"]
[5,"扬州北辰电气集团有限公司","绝缘手套","安全工器具","2019-12-01",{"$nulls":3},"工程一部"]
[6,"扬州北辰电气集团有限公司","绝缘手套","安全工器具","2019-12-01",{"$nulls":3},"工程一部"]
[7,"扬州北辰电气集团有限公司","绝缘靴","安全工器具","2019-12-01",{"$nulls":3},"工程一部"]
[8,"扬州北辰电气集团有限公司","绝缘靴","安全工器具","2019-12-01",{"$nulls":3},"工程一部"]
[9,"扬州北辰电气集团有限公司","绝缘靴","安全工器具","2019-12-01",{"$nulls":3},"工程一部"]
[10,"扬州北辰电气集团有限公司","绝缘靴","安全工器具","2019-12-01",{"$nulls":3},"工程一部"]
[11,"扬州北辰电气集团有限公司","绝缘靴","安全工器具","2019-12-01",{"$nulls":3},"工程一部"]
[12,"扬州北辰电气集团有限公司","绝缘靴","安全工器具","2019-12-01",{"$nulls":3},"工程一部"]
[13,"扬州北辰电气集团有限公司","绝缘安全带","安全工器具","2019-12-01",{"$nulls":3},"工程一部"]
[14,"扬州北辰电气集团有限公司","绝缘安全带","安全工器具","2019-12-01",{"$nulls":3},"工程一部"]
[15,"扬州北辰电气集团有限公司","绝缘安全带","安全工器具","2019-12-01",{"$nulls":3},"工程一部"]
[16,"扬州北辰电气集团有限公司","绝缘安全带","安全工器具","2019-12-01",{"$nulls":3},"工程一部"]
[17,"扬州北辰电气集团有限公司","绝缘安全带","安全工器具","2019-12-01",{"$nulls":3},"工程一部"]
[18,"扬州北辰电气集团有限公司","绝缘安全带","安全工器具","2019-12-01",{"$nulls":3},"工程一部"]
[19,"扬州北辰电气集团有限公司","绝缘手套","安全工器具","2019-12-01",{"$nulls":3},"工程一部"]
[20,"扬州北辰电气集团有限公司","绝缘手套","安全工器具","2019-12-01",{"$nulls":3},"工程一部"]
[21,"扬州北辰电气集团有限公司","绝缘手套","安全工器具","2019-12-01",{"$nulls":3},"工程一部"]
[22,"扬州北辰电气集团有限公司","绝缘手套","安全工器具","2019-12-01",{"$nulls":3},"工程一部"]
[23,"扬州北辰电气集团有限公司","绝缘手套","安全工器具","2019-12-01",{"$nulls":3},"工程一部"]
[24,"扬州北辰电气集团有限公司","绝缘手套","安全工器具","2019-12-01",{"$nulls":3},"工程一部"]
[25,"扬州北辰电气集团有限公司","绝缘安全帽","安全工器具","2019-12-01",{"$nulls":3},"工程一部"]
[26,"扬州北辰电气集团有限公司","绝缘安全帽","安全工器具","2019-12-01",{"$nulls":3},"工程一部"]
[27,"扬州北辰电气集团有限公司","绝缘安全帽","安全工器具","2019-12-01",{"$nulls":3},"工程一部"]
[28,"扬州北辰电气集团有限公司","绝缘安全帽","安全工器具","2019-12-01",{"$nulls":3},"工程一部"]
[29,"扬州北辰电气集团有限公司","绝缘安全帽","安全工器具","2019-12-01",{"$nulls":3},"工程一部"]
[30,"扬州北辰电气集团有限公司","绝缘安全帽","安全工器具","2019-12-01",{"$nulls":3},"工程一部"]
[31,"扬州北辰电气集团有限公司","验电器","安全工器具","2019-12-01",{"$nulls":3},"工程一部"]
[32,"扬州北辰电气集团有限公司","验电器","安全工器具","2019-12-01",{"$nulls":3},"工程一部"]
[33,"扬州北辰电气集团有限公司","放电棒","安全工器具","2020-07-01",{"$nulls":3},"工程一部"]
[34,"扬州北辰电气集团有限公司","放电棒","安全工器具","2020-07-01",{"$nulls":3},"工程一部"]
[35,"扬州北辰电气集团有限公司","安全围栏","安全工器具","2020-07-01",{"$nulls":3},"工程一部"]
[36,"扬州北辰电气集团有限公司","个人安保线","安全工器具","2020-07-01",{"$nulls":3},"工程一部"]
[37,"扬州北辰电气集团有限公司","标示牌","安全工器具","2020-07-01",{"$nulls":3},"工程一部"]
[38,"扬州北辰电气集团有限公司","警示牌","安全工器具","2020-07-01",{"$nulls":3},"工程一部"]
[39,"扬州北辰电气集团有限公司","绝缘靴","安全工器具","2021-03-01",{"$nulls":3},"质量管理部"]
[40,"扬州北辰电气集团有限公司","绝缘手套","安全工器具","2021-03-01",{"$nulls":3},"质量管理部"]
[41,"扬州北辰电气集团有限公司","10KV绝缘棒","安全工器具","2021-03-01",{"$nulls":3},"质量管理部"]
[42,"扬州北辰电气集团有限公司","20KV绝缘棒","安全工器具","2021-01-01",{"$nulls":3},"质量管理部"]